Project Name:	Regional
	Project Code:	REG	Site ID:	T98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	Tandanus Road 28KM north from highway and 5.4KM
	 north of Dillon Creek:
	Date Desc.:	04/03/70	Elevation:	 320 metres
	Map Ref.:	Sheet No. : 8057   1:100000	Rainfall:	610
	Northing/Long.:	145.833333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-20.05	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tf	Substrate Material:	Undisturbed soil core, Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	Yellow earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); Greyish brown (10YR5/2-Dry); ; Clay loam; Massive grade of
	 structure; Dry; Very firm consistence; Gradual change to - 
	A3	0.1 - 0.15 m	Yellowish brown (10YR5/4-Moist); Light yellowish brown (10YR6/4-Dry); ; Clay loam; Massive 
	grade of structure; Earthy fabric; Moderately moist; Firm consistence; 0-2%, coarse gravelly, 20-
	60mm, Quartz, coarse fragments; 
	B1	0.15 - 0.2 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 0-2%, coarse gravelly, 20-60mm, Quartz, coarse fragments; Very few (0 - 2 
	%), Unidentified, , Nodules; 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 0-2%, coarse gravelly, 20-60mm, Quartz, coarse fragments; Very few (0 - 2 
	%), Unidentified, , Nodules; 
	B21	0.3 - 0.4 m	Brownish yellow (10YR6/5-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 0-2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Gradual change 
	to - 
	B22	0.4 - 0.6 m	Light yellowish brown (2.5Y6/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Few (2 - 10 %), Unidentified, , Nodules; 
	B22	0.6 - 0.72 m	Light yellowish brown (2.5Y6/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Few (2 - 10 %), Unidentified, , Nodules; 
	0.72 - 0.9 m	Pale yellow (2.5Y7/4-Moist); , 10YR68, 2-10% , 5-15mm, Distinct; , 10YR81, 2-10% , 5-15mm, 
	Distinct; Light medium clay; Massive grade of structure; Earthy fabric; Weak consistence; Very 
	few (0 - 2 %), Unidentified, , Nodules; 
	D	0.9 - 1.2 m	Greyish brown (2.5Y5/2-Moist); , 10YR66; Heavy clay; Moderate grade of structure, 50-100 mm, 
	Angular blocky; Moderately moist; Rigid consistence; 
	D	1.2 - 1.5 m	Greyish brown (2.5Y5/2-Moist); , 10YR66; Heavy clay; Moderate grade of structure, 50-100 mm, 
	Angular blocky; Moderately moist; Rigid consistence; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	D	1.5 - 1.8 m	Greyish brown (2.5Y5/2-Moist); , 10YR66; Heavy clay; Moderate grade of structure, 50-100 mm, 
	Angular blocky; Moderately moist; Rigid consistence; 
	1.8 - 1.9 m	; 
	Morphological Notes
	Unconsolidated granitic material:
	Observation Notes
	90-120CM BLEACHED MATERIAL PRESENT ON TOP OF CLAY:90-180CM GREY COATINGS ON PED FACES:                       
	           
	Site Notes
	DILLON CK.

	Project Name:	Regional
	Project Code:	REG	Site ID:	T98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2A	 0.02A	 2.3B	 2.3	 0.53	 0.09	 1.1F	 6.3F
	0.1 - 0.15	6A	 0.02A	 1.8B	 1.9	 0.32	 0.1	 2.1F	 6.2F
	0.15 - 0.2	5.6A	 0.029A
	0.2 - 0.3	5.6A	 0.029A	 1.9B	 2.1	 0.19	 0.14	 1.6F	 5.9F
	0.3 - 0.4	5.8A	 0.026A	 1.9B	 2.7	 0.13	 0.18	 1.5F	 6.4F
	0.4 - 0.6	6.1A	 0.026A	 1.8B	 2.8	 0.08	 0.36	 1.5F	 6.5F
	0.6 - 0.72	6.2A	 0.02A
	0.72 - 0.9	6.5A	 0.032A	 1.4B	 3	 0.07	 0.3	 1.6F	 6.4F
	0.9 - 1.2	6.7A	 0.044A	 1.6B	 4.2	 0.07	 0.7	 0.7F	 7.3F
	1.2 - 1.5	7.8A	 0.107A
	1.5 - 1.8	9A	 0.226A
	1.8 - 2.1	9.4A	 0.282A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.46D	<2B	 0.011A	 0.05A	 0.27A	 2	 35A	 31	 11	 23
	0.1 - 0.15	 0.27D	<2B	 0.009A	 0.03A	 0.27A	 7	 29A	 31	 10	 29
	0.15 - 0.2	<2B
	0.2 - 0.3	<2B	 0.008A	 0.026A	 9	 37A	 24	 8	 31
	0.3 - 0.4	 25	 34A	 23	 8	 36
	0.4 - 0.6	 26	 32A	 22	 8	 39
	0.6 - 0.72
	0.72 - 0.9	 25	 44A	 16	 7	 33
	0.9 - 1.2	 18	 28A	 19	 8	 46
	1.2 - 1.5
	1.5 - 1.8	 10	 18A	 18	 10	 54
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.72
	0.72 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)