Project Name:	Regional
	Project Code:	REG	Site ID:	TL59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	Webb, Ian	Locality:
	Date Desc.:	//	Elevation:	 1100 metres
	Map Ref.:	Sheet No. : 7964   1:100000	Rainfall:	0
	Northing/Long.:	145.266666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-16.5	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	, Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	18 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	N/A
	Erosion:	Stable, 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Xanthozem
	Confidence level not specified
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Earthy fabric; Fine, (0 - 5) mm crack; Very weak consistence; 10-20%, fine gravelly, 2-
	6mm, subangular, undisturbed, Quartz, coarse fragments; AbundantAbrupt, Smooth change to - 
	0.05 - 0.1 m	Brown (10YR4/3-Moist); ; Loamy sand; Weak grade of structure, 10-20 mm, Subangular blocky; 
	Earthy fabric; Fine, (0 - 5) mm crack; Very weak consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular, undisturbed, Quartz, coarse fragments; AbundantClear, Smooth change to - 
	0.1 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Coarse sandy loam; Weak grade of structure, 10-20 
	mm, Subangular blocky; Earthy fabric; Fine, (0 - 5) mm crack; Weak consistence; 10-20%, fine 
	gravelly, 2-6mm, subangular, undisturbed, Quartz, coarse fragments; ManyGradual, Wavy 
	change to - 
	0.3 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Earthy fabric; Fine, (0 - 5) mm crack; Weak consistence; 10-20%, fine 
	gravelly, 2-6mm, subangular, undisturbed, Quartz, coarse fragments; CommonDiffuse, Irregular 
	change to - 
	0.6 - 0.9 m	Strong brown (7.5YR5/6-Moist); ; Clay loam; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Earthy fabric; Fine, (0 - 5) mm crack; Firm consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular, undisturbed, Quartz, coarse fragments; FewDiffuse, Irregular change to - 
	0.9 - 1.2 m	; Clay loam; Moderate grade of structure; Smooth-ped fabric; Firm consistence; 10-20%, fine 
	gravelly, 2-6mm, subangular, undisturbed, Quartz, coarse fragments; Few cutans, <10% of ped 
	faces or walls coated; Few (2 - 10 %), Ferruginous, Very coarse (20 - 60 mm), Soft segregations;
	 FewDiffuse, Irregular change to - 
	1.2 - 1.5 m	; Clay loam; Moderate grade of structure; Smooth-ped fabric; Very strong consistence; 20-50%, 
	medium gravelly, 6-20mm, angular, undisturbed, Granite, coarse fragments; Few cutans, <10% 
	of ped faces or walls coated; , Discontinuous; Few
	Morphological Notes
	Observation Notes
	WAS ORIGINALLY EP18:M3601-M3609:                                                                                        
	Site Notes
	Mt. Lewis

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	3.8D	 1.07H	 1.17	 0.59	 0.32	 8.45F	 4J	 11.6B	8.00
	4A	 5.15B
	3.8I	 3.3H
	0.05 - 0.1	4.2D	 0.17H	 0.24	 0.28	 0.16	 6.55F	 1.9J	 7.4B	8.42
	4.4A	 4.47B
	4.1I	 2.08H
	0.1 - 0.2	4.4A	 0.1H	 0.15	 0.16	 0.12	 1.48F	 1.9J	 2.01B	6.32
	4.2I	 1.36B
	 0.12H
	0.2 - 0.3	4.6A	 0.07H	 0.11	 0.17	 0.12	 1.04F	 1.5J	 1.51B	8.00
	4.2I	 1.04B
	0.3 - 0.6	4.5A	 0.07H	 0.05	 0.11	 0.09	 0.33F	 0.7J	 0.65B	12.86
	4.4I	 0.22B
	 0.11H
	0.6 - 0.9	4.4A	 0.03H	 0.05	 0.11	 0.09	 0.66F	 0.4J	 0.94B	22.50
	4.3I	 0.53B
	 0.13H
	0.9 - 1.2	4.4A	 0.05H	 0.05	 0.17	 0.08	 0.48F	 0.83B
	4.4I	 0.4B
	 0.08H
	1.2 - 1.5	4.4A	 0.03H	 0.05	 0.17	 0.09	 0.43F	 0J	 0.77B
	4.4I	 0.32B
	 0.11H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 8.43D
	0.05 - 0.1	 4.23D	1.10
	0.1 - 0.2	 3.84D
	0.2 - 0.3	 2.86D	1.30
	0.3 - 0.6	 1.64D
	0.6 - 0.9	 1.13D
	0.9 - 1.2	 0.82D
	1.2 - 1.5	 0.72D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P3A_NR	Bulk density - Not recorded