Project Name:	RR
	Project Code:	RR	Site ID:	B280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/56	Elevation:	 500 metres
	Map Ref.:	Sheet No. : 8064   1:100000	Rainfall:	2500
	Northing/Long.:	145.8575	Runoff:	Moderately rapid
	Easting/Lat.:	-16.9797222222222	Drainage:	Well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgm	Substrate Material:	Existing vertical exposure, 1.8 m 
	deep,Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Mountains
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Reddish brown (5YR4/4-Dry); ; Clay loam; Strong grade of structure, 2-5 mm, Granular; Many (>5 
	per 0.01m2) Coarse (>5mm) macropores, Dry; Weak consistence; 2-10%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Field pH 5.5 (pH meter); Abundant, fine (1-2mm) roots; Clear change 
	to - 
	A3	0.04 - 0.27 m	Yellowish red (5YR4/5-Dry); ; Clay loam (Heavy); Moderate grade of structure, 10-20 mm, 
	Polyhedral; Many (>5 per 0.01m2) Coarse (>5mm) macropores, Moderately moist; Weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.1 (pH meter); 
	Many, fine (1-2mm) roots; Gradual change to - 
	B11	0.28 - 0.48 m	Red (2.5YR5/8-Moist); ; Medium clay; Weak grade of structure, Polyhedral; Many (>5 per 0.01m2)
	 Coarse (>5mm) macropores, Moderately moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Field pH 5.3 (pH meter); Common, very fine (0-1mm) roots; Diffuse 
	change to - 
	B12	0.48 - 0.69 m	Red (2.5YR4/8-Moist); ; Medium clay; Weak grade of structure, Polyhedral; Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Firm consistence; 2-10%, fine gravelly, 
	2-6mm, Quartz, coarse fragments; Field pH 5.3 (pH meter); Common, very fine (0-1mm) roots; 
	Diffuse change to - 
	B21	0.69 - 1.14 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Many (>5 per 100mm2) Fine (1-
	2mm) macropores, Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Field pH 5.2 (pH meter); Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	1.14 - 1.47 m	Red (2.5YR5/8-Moist); ; Clay loam; Massive grade of structure; Many (>5 per 100mm2) Fine (1-
	2mm) macropores, Moderately moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Field pH 5.2 (pH meter); Few, very fine (0-1mm) roots; Diffuse change to - 
	B3	1.47 - 1.77 m	Red (2.5YR4/8-Moist); ; Clay loam; Massive grade of structure; Common (1-5 per 100mm2) Fine 
	(1-2mm) macropores, Moderately moist; Firm consistence; 10-20%, fine gravelly, 2-6mm, Quartz,
	 coarse fragments; Field pH 5.1 (pH meter); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	RR
	Project Code:	RR	Site ID:	B280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	MURRAY PRIOR R

	Project Name:	RR
	Project Code:	RR	Site ID:	B280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.5H	 0.04B
	0.04 - 0.27	5.1H	 0.02B
	0.28 - 0.48	5.3H	 0.01B
	0.48 - 0.69	5.3H	 0.01B
	0.69 - 1.14	5.2H	 0.01B
	1.14 - 1.47	5.2H	 0.01B
	1.47 - 1.77	5.1H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 6C	 0.034F	1.00	 7	 51C	 12	 15	 20
	0.04 - 0.27	 0.024F	1.30	 13	 46C	 13	 16	 27
	0.28 - 0.48	 0.7A	 0.022F	1.40	 9	 35C	 11	 12	 38
	0.48 - 0.69	 0.022F	1.40	 11	 39C	 11	 14	 35
	0.69 - 1.14	 0.002F	1.40
	1.14 - 1.47	 0.021F	1.40	 13	 50C	 15	 12	 23
	1.47 - 1.77	 0.037F	1.50	 12	 36C	 21	 21	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04	 0.23C	 0.19C
	0.04 - 0.27	 0.28C	 0.22C
	0.28 - 0.48	 0.32C	 0.24C
	0.48 - 0.69	 0.33C	 0.26C
	0.69 - 1.14	 0.32C	 0.26C
	1.14 - 1.47	 0.3C	 0.23C
	1.47 - 1.77	 0.3C	 0.22C

	Project Name:	RR
	Project Code:	RR	Site ID:	B280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate