Project Name:	RR
	Project Code:	RR	Site ID:	B500	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	13/09/63	Elevation:	 137 metres
	Map Ref.:	Sheet No. : 8950   1:100000	Rainfall:	707
	Northing/Long.:	150.117777777778	Runoff:	Rapid
	Easting/Lat.:	-23.6625	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.64 m deep,Igneous rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	30 metres
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	8.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Red Vertosol     	Principal Profile Form:	Gn3.13
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - Heteropogon contortus
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus dichromophloia
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, angular, Igneous rock (unidentified)
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Light clay (Heavy); Moderate grade of structure, 5-10 mm, 
	Polyhedral; Many (>5 per 0.01m2) Medium (2-5mm) macropores, Moderately moist; Firm 
	consistence; 2-10%, medium gravelly, 6-20mm, angular, coarse fragments; Field pH 6.6 (pH 
	meter); Clear change to - 
	B21	0.1 - 0.36 m	Red (2.5YR4/5-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, Polyhedral; 
	Moist; Firm consistence; 2-10%, medium gravelly, 6-20mm, coarse fragments; Field pH 7 (pH 
	meter); Clear change to - 
	B22	0.36 - 0.53 m	Dark reddish brown (5YR3/4-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, 
	Polyhedral; Dry; Strong consistence; 2-10%, medium gravelly, 6-20mm, coarse fragments; Very 
	few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Field pH 7.9 (pH meter); Clear change to - 
	B3	0.53 - 0.64 m	Yellowish red (5YR3/5-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, 
	Lenticular; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Few (2 - 10 
	%), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.7 (pH meter); Gradual change to - 
	C1	0.64 - 0.84 m	Reddish brown (5YR4/3-Moist); , 5Y62; , 10YR82; Light clay (Heavy); Massive grade of structure;
	 Moderately moist; Firm consistence; 2-10%, Substrate material, coarse fragments; Field pH 8.9
	 (pH meter); Gradual change to - 
	C2	0.84 - 1.07 m	; Field pH 8.8 (pH meter); 
	Morphological Notes
	C2	Weathered rock.
	Observation Notes
	MOTTLED RB(5YR4/3) WHITE AND GREY WEATHERED ROCK.                                                                       
	Site Notes
	WESTWOOD

	Project Name:	RR
	Project Code:	RR	Site ID:	B500	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6H	 0.02B	 11.2K	 8.5	 0.19	 0.04	 11.3D
	0.1 - 0.36	7H	 0.02B	 17.3K	 13.6	 0.06	 0.41	 7.4D
	0.36 - 0.53	7.9H	 0.02B	 16.8K	 13.9	 0.04	 0.6	 6.6D
	0.53 - 0.64	8.7H	 0.06B	 14.7K	 12.2	 0.02	 0.59	 5D
	0.64 - 0.84	8.9H	 0.05B
	0.84 - 1.07	8.8H	 0.03B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.64A	 4C	 0.033F	 0.164B	 6	 9C	 27	 19	 41
	0.1 - 0.36	 0.83A	 0.02F	 0.084B	 6	 5C	 20	 14	 58
	0.36 - 0.53	 0.1C	 0.57A	 0.028F	 0.061B	 6	 9C	 22	 16	 51
	0.53 - 0.64	 6.4C	 0.47A	 0.05F	 0.051B	 7	 7C	 28	 15	 38
	0.64 - 0.84	 7.9C	 0.09F	 16	 13C	 39	 16	 21
	0.84 - 1.07	 0.1C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.36
	0.36 - 0.53
	0.53 - 0.64
	0.64 - 0.84
	0.84 - 1.07

	Project Name:	RR
	Project Code:	RR	Site ID:	B500	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded