Project Name:	RR
	Project Code:	RR	Site ID:	B555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	07/09/66	Elevation:	 305 metres
	Map Ref.:	Sheet No. : 9044   1:100000	Rainfall:	690
	Northing/Long.:	150.6	Runoff:	No runoff
	Easting/Lat.:	-26.7166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	9 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Tall Strata - Tree, , Isolated plants. *Species includes - Acacia harpophylla, Brachychiton rupestre
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; 5-10 mm, Angular blocky; Wet; Very plastic; 0-2%, coarse gravelly, 20-60mm, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 7 (pH 
	meter); Gradual change to - 
	A1	0.1 - 0.2 m	Dark grey (10YR4/1-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; 5-10 mm, Angular blocky; Wet; Very plastic; 0-2%, coarse gravelly, 20-60mm, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 7.7 (pH 
	meter); 
	A1	0.2 - 0.3 m	Dark grey (10YR4/1-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; 5-10 mm, Angular blocky; Wet; Very plastic; 0-2%, coarse gravelly, 20-60mm, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 8.2 (pH 
	meter); Gradual change to - 
	B2	0.3 - 0.45 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Angular blocky;
	 5-10 mm, Angular blocky; Wet; Very plastic; 0-2%, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; Field pH 7.8 (pH meter); 
	B2	0.45 - 0.6 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Angular blocky;
	 5-10 mm, Angular blocky; Wet; Very plastic; 0-2%, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; Field pH 6.1 (pH meter); Diffuse change to - 
	B2	0.6 - 0.9 m	Grey (10YR5/1-Moist); ; Medium heavy clay; 50-100 mm, Angular blocky; Moderate grade of 
	structure, 10-20 mm, Angular blocky; Moist; Firm consistence; 0-2%, Quartz, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, , Nodules; Field pH 6 (pH meter); 
	B2	0.9 - 1.2 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Moderate grade of structure, 50-100 mm, Angular 
	blocky; 10-20 mm, Angular blocky; Moist; Firm consistence; 0-2%, Quartz, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, , Nodules; Field pH 6 (pH meter); 
	B2	1.2 - 1.5 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Nodules; Field pH 6.8 (pH meter); 

	Project Name:	RR
	Project Code:	RR	Site ID:	B555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	1.5 - 1.8 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Nodules; Field pH 7.2 (pH meter); 
	B2	1.8 - 2.1 m	Grey (10YR5/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Nodules; 
	B2	2.1 - 2.4 m	Grey (10YR6/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Soft segregations; 
	B2	2.4 - 2.6 m	Grey (10YR6/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Soft segregations; 
	B2	2.6 - 2.8 m	Grey (10YR6/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, , 
	Soft segregations; Diffuse change to - 
	B3	2.8 - 2.95 m	Grey (10YR6/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; 0-2%, Silcrete, coarse fragments; 
	B3	2.95 - 3.1 m	Grey (10YR6/1-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 mm, 
	Lenticular; 20-50 mm, Lenticular; Moist; Firm consistence; 0-2%, Silcrete, coarse fragments; 
	Clear change to - 
	C	3.1 - 3.3 m	; 
	Morphological Notes
	C	W(10YR92)with GB&PY patch';weat'd siltstone with clay veins
	Observation Notes
	(10YR 9/2) WITH GB & PY PATCHES; WEATHERED SILTSTONE WITH CLAY VEINS.                                                   
	Site Notes
	CHINCHILA

	Project Name:	RR
	Project Code:	RR	Site ID:	B555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7A	 0.1A	 17B	 6.6	 1.4	 1.4	 0.1D
	0.1 - 0.2	7.7A	 0.14A
	0.2 - 0.3	8.2A	 0.22A	 15.1B	 9.4	 0.88	 4.5	 0D
	0.3 - 0.45	7.8A	 0.49A	 11.1B	 9.4	 0.83	 5.6	 0D
	0.45 - 0.6	6.1A	 0.89A	 7B	 7.8	 0.72	 6.1	 0.65D
	0.6 - 0.9	6A	 1.24A	 4.6B	 7.3	 0.61	 5.6	 3.8D
	0.9 - 1.2	6A	 1.54A
	1.2 - 1.5	6.8A	 1.68A	 4.5B	 12	 0.96	 8.8	 0D
	1.5 - 1.8	7.2A	 1.97A
	1.8 - 2.1	7.5A	 1.97A
	2.1 - 2.4	7.1A	 2.11A
	2.4 - 2.6	7.2A	 1.97A
	2.6 - 2.8
	2.8 - 2.95	6.9A	 1.95A
	2.95 - 3.1	6.8A	 2.16A
	3.1 - 3.3	6.8A	 2.11A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.68A	 50A	 0.031A	 0.13B	 0.44A	1.15	 1	 3C	 26	 6	 60
	 43B
	0.1 - 0.2	 0.088B	1.37
	0.2 - 0.3	 0.81A	 0.015A	 0.071B	 0.4A	 1	 3C	 28	 17	 50
	0.3 - 0.45	 0.7A	 0.014A	 0.059B	 0.4A	1.52	 1	 3C	 29	 17	 49
	0.45 - 0.6	 0.52A	 0.013A	 0.044B	 0.39A	1.54	 1	 3C	 28	 16	 49
	0.6 - 0.9	 0.012A	 0.04B	 0.39A	1.59	 1	 3C	 30	 14	 51
	0.9 - 1.2
	1.2 - 1.5	 0.012A	 0.03B	 0.4A	 1	 7C	 26	 14	 52
	1.5 - 1.8	 0.014A	 0.44A	 1	 2C	 28	 15	 52
	1.8 - 2.1
	2.1 - 2.4	 1	 2C	 26	 16	 54
	2.4 - 2.6
	2.6 - 2.8
	2.8 - 2.95
	2.95 - 3.1
	3.1 - 3.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.37F	0.22H
	0.1 - 0.2	0.39F	0.29H
	0.2 - 0.3
	0.3 - 0.45	0.38F	0.28H
	0.45 - 0.6	0.38F	0.27H
	0.6 - 0.9	0.39F	0.29H
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	RR
	Project Code:	RR	Site ID:	B555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.6
	2.6 - 2.8
	2.8 - 2.95
	2.95 - 3.1
	3.1 - 3.3

	Project Name:	RR
	Project Code:	RR	Site ID:	B555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B3VLe004	0.04 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe03	0.3 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe06	0.6 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe15	15 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe2	2 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe7	7 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate