Project Name:	RR
	Project Code:	RR	Site ID:	B564	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	21/10/66	Elevation:	 27 metres
	Map Ref.:	Sheet No. : 9348   1:100000	Rainfall:	1105
	Northing/Long.:	152.4	Runoff:	Rapid
	Easting/Lat.:	-24.85	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czub	Substrate Material:	Undisturbed soil core, 2.1 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Ferrosol     	Principal Profile Form:	Uf5.21
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, 
	Polyhedral; <2 mm, Angular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, Dry; Firm
	 consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 6.8 (pH 
	meter); 
	A1	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, 
	Polyhedral; <2 mm, Angular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, Dry; Firm
	 consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 6.8 (pH 
	meter); Diffuse change to - 
	B21	0.2 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; <2 mm, Angular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, 
	Moderately moist; Weak consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Field pH 6.8 (pH meter); 
	B21	0.3 - 0.6 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Strong grade of structure, 10-20 mm, 
	Polyhedral; <2 mm, Angular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, 
	Moderately moist; Weak consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Field pH 6.8 (pH meter); 
	B21	0.6 - 0.9 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Strong grade of structure, 10-20 mm, 
	Polyhedral; <2 mm, Angular blocky; Many (>5 per 0.01m2) Coarse (>5mm) macropores, 
	Moderately moist; Weak consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Field pH 7 (pH meter); Diffuse change to - 
	B22	0.9 - 1.2 m	Reddish brown (2.5YR4/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; 5-10 mm, Angular blocky; Moist; Very weak consistence; 0-2%, Basalt, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 7 (pH 
	meter); 
	B22	1.2 - 1.5 m	Reddish brown (2.5YR4/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; 5-10 mm, Angular blocky; Moist; Very weak consistence; 0-2%, Basalt, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 7 (pH 
	meter); 

	Project Name:	RR
	Project Code:	RR	Site ID:	B564	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	1.5 - 1.8 m	Reddish brown (2.5YR4/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; 5-10 mm, Angular blocky; Moist; Very weak consistence; 0-2%, Basalt, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Field pH 6.6 (pH 
	meter); Diffuse change to - 
	B3	1.8 - 2 m	Yellowish red (5YR4/6-Moist); , 10YR56, 10-20% , 5-15mm, Faint; , 10YR64, 10-20% , 5-15mm, 
	Faint; Light clay; Moderate grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Few 
	(<1 per 0.01m2) Coarse (>5mm) macropores, Moist; Very weak consistence; 0-2%, coarse 
	gravelly, 20-60mm, Basalt, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 
	mm), Nodules; Field pH 6.3 (pH meter); 
	B3	2 - 2.1 m	Yellowish red (5YR4/6-Moist); , 10YR56, 10-20% , 5-15mm, Faint; , 10YR64, 10-20% , 5-15mm, 
	Faint; Light clay; Moderate grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Few 
	(<1 per 0.01m2) Coarse (>5mm) macropores, Moist; Very weak consistence; 0-2%, coarse 
	gravelly, 20-60mm, Basalt, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 
	mm), Nodules; Field pH 6.2 (pH meter); 
	C	2.1 - 2.43 m	Light yellowish brown (10YR6/4-Moist); , 5YR56, 20-50% , 15-30mm, Distinct; , 2.5Y71, 20-50% 
	, 15-30mm, Distinct; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; Moist; 
	Weak consistence; 10-20%, cobbly, 60-200mm, Basalt, coarse fragments; Field pH 6 (pH 
	meter); Abrupt change to - 
	2.43 - 2.7 m	Brown (10YR5/3-Moist); , 7.5YR44, 20-50% , 15-30mm, Prominent; , 7.5YR22, 20-50% , 15-
	30mm, Prominent; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; Weak 
	consistence; 2-10%, cobbly, 60-200mm, Basalt, coarse fragments; Field pH 5.9 (pH meter); 
	2.7 - 3 m	Brown (10YR5/3-Moist); , 7.5YR44, 20-50% , 15-30mm, Prominent; , 7.5YR22, 20-50% , 15-
	30mm, Prominent; Light medium clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Weak consistence; 2-10%, cobbly, 60-200mm, Basalt, coarse fragments; Field pH 5.8 (pH 
	meter); Diffuse change to - 
	3 - 3.3 m	Brown (10YR5/3-Moist); , 7.5YR44, 20-50% , 15-30mm, Prominent; , 7.5YR46, 20-50% , 15-
	30mm, Prominent; Light clay; Massive grade of structure; Weak consistence; 20-50%, cobbly, 
	60-200mm, Basalt, coarse fragments; Field pH 5.6 (pH meter); 
	3.3 - 3.6 m	Brown (10YR5/3-Moist); , 7.5YR44, 20-50% , 15-30mm, Prominent; , 7.5YR46, 20-50% , 15-
	30mm, Prominent; Light clay; Massive grade of structure; Weak consistence; 20-50%, cobbly, 
	60-200mm, Basalt, coarse fragments; Field pH 5.5 (pH meter); 
	Morphological Notes
	Observation Notes
	SUGAR EXPERIMENTAL STATION.                                                                                             
	Site Notes
	BUNDABERG

	Project Name:	RR
	Project Code:	RR	Site ID:	B564	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.8A	 0.054A	 7.4B	 3	 1.9	 0.17	 1.7D
	0.1 - 0.2	6.8A	 0.043A	 6.1B	 2.3	 1.6	 0.21	 0.55D
	0.2 - 0.3	6.8A	 0.054A	 5.5B	 2	 1.9	 0.07	 0.27D
	0.3 - 0.6	6.8A	 0.097A	 4.5B	 1.2	 1.9	 0.12	 0.76D
	0.6 - 0.9	7A	 0.114A	 3.7B	 1.1	 2.2	 0.02	 0D
	0.9 - 1.2	7A	 0.111A
	1.2 - 1.5	7A	 0.108A	 2.6B	 0.6	 2	 0.17	 0D
	1.5 - 1.8	6.6A	 0.119A	 1.9B	 0.9	 2.2	 0.22	 0.18D
	1.8 - 2	6.3A	 0.13A
	2 - 2.1	6.2A	 0.141A
	2.1 - 2.43	6A	 0.146A	 2.7B	 0.45	 3	 0.34	 3.7D
	2.43 - 2.7	5.9A	 0.105A
	2.7 - 3	5.8A	 0.073A	 4.6B	 0.72	 1.6	 0.7	 2.4D
	3 - 3.3	5.6A	 0.059A	 4.8B	 1.1	 1	 0.8	 3.4D
	3.3 - 3.6	5.5A	 0.065A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.38A	 160A	 0.37A	 0.24B	 0.2A	1.38	 11	 19C	 9	 10	 58
	 110B
	0.1 - 0.2	 1.86A	 69A	 0.26A	 0.2B	 0.19A	 5	 14C	 8	 10	 64
	 40B
	0.2 - 0.3	 1.57A	 49A	 0.23A	 0.18B	 0.2A	1.53	 1	 11C	 8	 10	 68
	 25B
	0.3 - 0.6	 0.87A
	0.6 - 0.9	 0.19A	 0.071B	 0.19A	 3	 11C	 18	 25	 48
	0.9 - 1.2
	1.2 - 1.5	 0.23A	 0.043B	 0.2A	 8	 18C	 14	 21	 47
	1.5 - 1.8	 0.21A	 0.037B	 0.22A	 15	 14C	 11	 22	 56
	1.8 - 2
	2 - 2.1	 2	 10C	 11	 29	 51
	2.1 - 2.43	 21	 6C	 12	 30	 54
	2.43 - 2.7
	2.7 - 3	 12	 3C	 8	 26	 64
	3 - 3.3
	3.3 - 3.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.41F	0.28H
	0.1 - 0.2
	0.2 - 0.3	0.4F	0.31H
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8

	Project Name:	RR
	Project Code:	RR	Site ID:	B564	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2
	2 - 2.1
	2.1 - 2.43
	2.43 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6

	Project Name:	RR
	Project Code:	RR	Site ID:	B564	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B3VLe004	0.04 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe03	0.3 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe06	0.6 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe15	15 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe2	2 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe7	7 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate