Project Name:	RR
	Project Code:	RR	Site ID:	B566	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	22/10/66	Elevation:	 3 metres
	Map Ref.:	Sheet No. : 9348   1:100000	Rainfall:	1105
	Northing/Long.:	152.333333333333	Runoff:	Very slow
	Easting/Lat.:	-24.7666666666667	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Undisturbed soil core, 1 m 
	deep,Unconsolidated material 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	2 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Gn3.41
	ASC Confidence:	Great Soil Group:	Humic gley
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Sod grass, 0.26-0.5m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, 
	Granular; Moist; Very weak consistence; Field pH 5.8 (pH meter); Many, fine (1-2mm) roots; 
	Abrupt change to - 
	B2	0.05 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); , 5YR33, 20-50% , 0-5mm, Distinct; , 7.5YR58, 20-50%
	 , 0-5mm, Distinct; Light clay; Strong grade of structure, 20-50 mm, Prismatic; 10-20 mm, 
	Angular blocky; Moist; Firm consistence; Field pH 5.6 (pH meter); Many, fine (1-2mm) roots; 
	B2	0.1 - 0.2 m	Very dark greyish brown (10YR3/2-Moist); , 5YR33, 20-50% , 0-5mm, Distinct; , 7.5YR58, 20-50%
	 , 0-5mm, Distinct; Light clay; Strong grade of structure, 20-50 mm, Prismatic; 10-20 mm, 
	Angular blocky; Moist; Firm consistence; Field pH 5.6 (pH meter); Common, fine (1-2mm) roots; 
	B2	0.2 - 0.27 m	Very dark greyish brown (10YR3/2-Moist); , 5YR33, 20-50% , 0-5mm, Distinct; , 7.5YR58, 20-50%
	 , 0-5mm, Distinct; Light clay (Heavy); Strong grade of structure, 20-50 mm, Prismatic; 10-20 
	mm, Angular blocky; Moist; Firm consistence; Field pH 5.3 (pH meter); Common, fine (1-2mm) 
	roots; Diffuse change to - 
	B2	0.27 - 0.3 m	Very dark greyish brown (10YR3/2-Moist); , 7.5YR58, 20-50% , 0-5mm, Distinct; , 5YR33, 20-50%
	 , 0-5mm, Distinct; Light medium clay; Strong grade of structure, 20-50 mm, Prismatic; 10-20 
	mm, Angular blocky; Moist; Firm consistence; Very few (0 - 2 %), Ferromanganiferous, , Soft 
	segregations; Field pH 5.2 (pH meter); Few, fine (1-2mm) roots; 
	B2g	0.3 - 0.43 m	Grey (2.5Y5/1-Moist); , 10YR66, 20-50% , 0-5mm, Prominent; , 10R46, 20-50% , 0-5mm, 
	Prominent; Medium clay; Moderate grade of structure, 20-50 mm, Prismatic; 10-20 mm, Angular 
	blocky; Moist; Moderately plastic; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Field pH 
	5.1 (pH meter); 
	B2g	0.43 - 0.61 m	Grey (2.5Y5/1-Moist); , 10YR66, 20-50% , 5-15mm, Prominent; , 10R46, 20-50% , 5-15mm, 
	Prominent; Medium clay; Moderate grade of structure, 20-50 mm, Prismatic; 10-20 mm, Angular 
	blocky; Moist; Moderately plastic; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Field pH 
	4.8 (pH meter); 

	Project Name:	RR
	Project Code:	RR	Site ID:	B566	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2g	0.61 - 0.66 m	Grey (2.5Y5/1-Moist); , 10YR66, 20-50% , 5-15mm, Prominent; , 10R46, 20-50% , 5-15mm, 
	Prominent; Medium clay; Moderate grade of structure, 20-50 mm, Prismatic; 10-20 mm, Angular 
	blocky; Moist; Moderately plastic; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Field pH 
	4.8 (pH meter); 
	B2g	0.66 - 0.84 m	Grey (2.5Y5/1-Moist); , 10YR66, 20-50% , 5-15mm, Prominent; , 10R46, 20-50% , 5-15mm, 
	Prominent; Medium clay; Moderate grade of structure, 20-50 mm, Prismatic; 10-20 mm, Angular 
	blocky; Moist; Moderately plastic; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Field pH 
	4.9 (pH meter); Diffuse change to - 
	B3g	0.84 - 0.92 m	 (N4/0-Moist); , 10YR66, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; Light medium 
	clay; Weak grade of structure, 20-50 mm, Prismatic; 10-20 mm, Angular blocky; Moist; 
	Moderately plastic; Field pH 5.2 (pH meter); 
	Morphological Notes
	Observation Notes
	0-5CM POROUS GRANULAR STRUCTURE:PARENT MATERIAL ESTURINE - MARINE SEDIMENTS:                                        
	    
	Site Notes
	BUNDABERG

	Project Name:	RR
	Project Code:	RR	Site ID:	B566	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.8H	 0.041B	 5.2K	 8.6	 3.4	 1.2	 16.2D
	0.05 - 0.1	5.6H	 0.029B	 4K	 8.6	 2.6	 1.7	 16.1D
	0.1 - 0.2	5.6H	 0.035B	 2.6K	 6.8	 1.8	 1.9	 16.2D
	0.2 - 0.27	5.3H	 0.05B
	0.27 - 0.3	5.2H	 0.059B
	0.3 - 0.43	5.1H	 0.086B
	0.43 - 0.61	4.8H	 0.128B	 1.7K	 7.7	 1	 3.7	 9.1D
	0.61 - 0.66	4.8H	 0.128B
	0.66 - 0.84	4.9H	 0.136B
	0.84 - 0.92	5.2H	 0.122B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 7.4E	 200C	 0.118F	 1.36B	0.74	 2C	 21	 29	 36
	 54B
	0.05 - 0.1	 4.3E	 51C	 0.061F	 1.44B	1.20	 1C	 14	 34	 46
	 30B
	0.1 - 0.2	 2.8E	 15C	 0.035F	 1.43B	 0C	 9	 34	 54
	 12B
	0.2 - 0.27
	0.27 - 0.3
	0.3 - 0.43	1.40
	0.43 - 0.61	 0.62E	 0.061F	 1.42B	 5C	 22	 24	 46
	0.61 - 0.66
	0.66 - 0.84
	0.84 - 0.92
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	 0.35C	 0.24C
	0.05 - 0.1	 0.43C	 0.32C
	0.1 - 0.2
	0.2 - 0.27
	0.27 - 0.3
	0.3 - 0.43	 0.46C	 0.34C
	0.43 - 0.61
	0.61 - 0.66
	0.66 - 0.84
	0.84 - 0.92

	Project Name:	RR
	Project Code:	RR	Site ID:	B566	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate