Project Name:	TBL
	Project Code:	TBL	Site ID:	B815	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	B. Slater	Locality:
	Date Desc.:	19/02/87	Elevation:	No Data
	Map Ref.:	Sheet No. : 8943   1:100000	Rainfall:	0
	Northing/Long.:	150.466666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-27.3833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic-Endoacidic Self-Mulching Grey Vertosol     	Principal Profile Form:	UG5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Mid Strata - , , . *Species includes - Geijera parviflora
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Casuarina cristata, Acacia harpophylla
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.04 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Light medium clay; Strong grade of 
	structure, <2 mm, Granular; Very weak consistence; Field pH 8.5 (pH meter); Clear change to - 
	0.04 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Angular blocky; Strong grade of structure, 5-10 mm, Angular blocky; Weak consistence; Clear 
	change to - 
	0.1 - 0.2 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44; Medium heavy clay; Moderate grade of structure,
	 10-20 mm, Angular blocky; Moderate grade of structure, 5-10 mm, Angular blocky; Strong 
	consistence; Gradual change to - 
	0.2 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint;
	 Medium heavy clay; Moderate grade of structure, 20-50 mm, Lenticular; Very strong 
	consistence; Field pH 8.9 (pH meter); Gradual change to - 
	0.3 - 0.38 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint;
	 Medium heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; 
	Gradual change to - 
	0.38 - 0.52 m	Dark grey (2.5Y4/1-Moist); , 7.5YR44, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint; Medium 
	heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; Very few (0
	 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Gradual change to - 
	0.52 - 0.6 m	Dark greyish brown (2.5Y4/2-Moist); , 7.5YR44, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; 
	Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Nodules; Field pH 9 (pH meter); Gradual change to 
	- 
	0.6 - 0.72 m	Greyish brown (10YR5/2-Moist); , 7.5YR46, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; 
	Gradual change to - 
	0.72 - 0.9 m	Brown (7.5YR5/2-Moist); , 7.5YR46, 0-2% , 15-30mm, Faint; , 0-2% , 15-30mm, Faint; Medium 
	heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; Field pH 
	4.5 (pH meter); Gradual change to - 

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B815	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.9 - 1.2 m	Brown (7.5YR5/3-Moist); , 5YR46, 2-10% , 15-30mm, Faint; , 2-10% , 15-30mm, Faint; Medium 
	heavy clay; Moderate grade of structure, 50-100 mm, Lenticular; Strong consistence; Field pH 4 
	(pH meter); Gradual change to - 
	1.2 - 1.5 m	Pinkish grey (7.5YR6/3-Moist); , 5YR46, 2-10% , 15-30mm, Faint; , 2-10% , 15-30mm, Faint; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Strong consistence; 
	Field pH 3.5 (pH meter); Gradual change to - 
	1.5 - 1.8 m	Pinkish grey (7.5YR6/3-Moist); , 5YR48, 2-10% , 15-30mm, Faint; , 2-10% , 15-30mm, Faint; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Strong consistence; 
	Morphological Notes
	Observation Notes
	LAYERS RENUMBERED 8-10-92                                                                                               
	Site Notes
	TARA

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B815	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	7.3H	 0.036B	 19.2K	 4.6	 2.7	 0.3	 2.9D
	0.04 - 0.1	8.1H	 0.029B	 21.6K	 4	 1.3	 0.5	 2.8D
	0.1 - 0.2	8.7H	 0.05B	 20.4K	 5.9	 0.8	 1.1	 2.7D
	0.2 - 0.3	9H	 0.078B	 17.8K	 7.4	 0.4	 2	 1.1D
	0.38 - 0.52	8.8H	 0.34B	 13.5K	 9.9	 0.5	 4.6	<0.1D
	0.6 - 0.72	8H	 0.59B	 10.3K	 11.3	 0.6	 7.2	<0.1D
	0.72 - 0.9	5.8H	 0.8B	 7.8K	 11.2	 0.6	 7.2	 1D
	0.9 - 1.2	4.6H	 0.53B	 6.1K	 9.9	 0.6	 7.6	 3.5D
	1.5 - 1.8	4.4H	 0.59B	 5.1K	 9.9	 0.6	 7.2	 7.4D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 2.63A	 27B	 0.036F	 0.27B	 0.44B	 12C	 34	 12	 36
	0.04 - 0.1	 1.46A	 8B	 0.031F	 0.174B	 0.36B	 11C	 33	 11	 39
	0.1 - 0.2	 0.83A	 9B	 0.026F	 0.097B	 0.31B	 11C	 30	 10	 44
	0.2 - 0.3	 0.58A	 13B	 0.016F	 0.073B	 0.29B	 10C	 28	 12	 42
	0.38 - 0.52	 0.009F	 0.042B	 0.29B	 12C	 32	 12	 44
	0.6 - 0.72	 0.01F	 0.05B	 0.3B	 10C	 32	 11	 46
	0.72 - 0.9	 0.008F	 0.045B	 0.29B	 11C	 28	 11	 48
	0.9 - 1.2	 0.007F	 0.031B	 0.3B
	1.5 - 1.8	 0.007F	 0.034B	 0.3B	 8C	 25	 14	 54
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.38 - 0.52
	0.6 - 0.72
	0.72 - 0.9
	0.9 - 1.2
	1.5 - 1.8

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B815	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded