Project Name:	TBL
	Project Code:	TBL	Site ID:	B831	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	B. Slater	Locality:
	Date Desc.:	25/02/87	Elevation:	No Data
	Map Ref.:	Sheet No. : 8943   1:100000	Rainfall:	0
	Northing/Long.:	150.216666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-27.4666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust, Hardsetting
	Erosion:	Moderate (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epiacidic Epipedal Brown Vertosol     	Principal Profile Form:	Ug5.34
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Sclerolaeana tetracuspis
	Tall Strata - , , . *Species includes - Acacia harpophylla
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, subrounded, Substrate material
	Profile Morphology
	A11	0 - 0.04 m	Brown (7.5YR4/3-Moist); Pinkish grey (7.5YR7/3-Dry); ; Light clay; Weak grade of structure, 2-
	5 mm, Angular blocky; Weak grade of structure, <2 mm, Granular; Moderately moist; Firm 
	consistence; Field pH 6.2 (pH meter); Clear change to - 
	A12	0.04 - 0.1 m	Brown (7.5YR4/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moderate grade of structure, 5-10 mm, Angular blocky; Dry; Very strong consistence; 
	Clear change to - 
	B21	0.1 - 0.2 m	Brown (7.5YR4/3-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Lenticular; 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; 
	Gradual change to - 
	B22	0.2 - 0.3 m	Brown (7.5YR4/3-Moist); ; Medium heavy clay; Moderate grade of structure, 50-100 mm, 
	Lenticular; 20-50 mm, Lenticular; Smooth-ped fabric; Dry; Very strong consistence; Field pH 4.8 
	(pH meter); Gradual change to - 
	B23	0.3 - 0.6 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; Moderate grade of structure, 50-100 mm, 
	Lenticular; 20-50 mm, Lenticular; Smooth-ped fabric; Dry; Very strong consistence; 0-2%, 
	medium gravelly, 6-20mm, subangular, Quartz, coarse fragments; Field pH 4.5 (pH meter); 
	Gradual change to - 
	B24	0.6 - 0.9 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; 50-100 mm, Lenticular; Smooth-ped fabric; Dry; 
	Very strong consistence; Field pH 4 (pH meter); Gradual change to - 
	B25	0.9 - 1.2 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; 50-100 mm, Lenticular; Smooth-ped fabric; Dry; 
	Very strong consistence; Field pH 4 (pH meter); Gradual change to - 
	1.2 - 1.5 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; 50-100 mm, Lenticular; Smooth-ped fabric; Very 
	strong consistence; Field pH 3.8 (pH meter); Gradual change to - 
	1.5 - 1.7 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; 50-100 mm, Lenticular; Smooth-ped fabric; Very 
	strong consistence; Field pH 3.7 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B831	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	TARA
	LAYERS RE NUMBERED 12/10/92                                                                                             

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B831	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5H	 0.25B	 12.2K	 7.4	 0.9	 1.4	 11.2D
	0.04 - 0.1	4.8H	 0.25B	 12.3K	 7.4	 0.7	 1.4	 12.6D
	0.1 - 0.2	4.6H	 0.28B	 10.8K	 8	 0.6	 1.6	 19.6D
	0.2 - 0.3	4.4H	 0.3B	 9.6K	 8.5	 0.4	 2.2	 12.8D
	0.3 - 0.6	4.4H	 0.39B	 8.8K	 9.7	 0.3	 3.5	 11.5D
	0.6 - 0.9	4.2H	 0.55B	 7.4K	 10	 0.2	 5	 11.3D
	0.9 - 1.2	4.1H	 0.6B	 6.3K	 9.6	 0.2	 5.6	 10.5D
	1.5 - 1.7	4.2H	 0.71B	 5.3K	 8.9	 0.3	 5.7	 10.4D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.47A	 14B	 0.018F	 0.149B	 0.18B	 2C	 25	 10	 58
	0.04 - 0.1	 1.37A	 11B	 0.018F	 0.135B	 0.18B	 2C	 26	 10	 59
	0.1 - 0.2	 1.02A	 8B	 0.015F	 0.118B	 0.17B	 3C	 25	 10	 59
	0.2 - 0.3	 0.81A	 6B	 0.015F	 0.099B	 0.16B	 2C	 25	 11	 60
	0.3 - 0.6	 0.012F	 0.078B	 0.15B	 2C	 23	 10	 63
	0.6 - 0.9	 0.01F	 0.064B	 0.14B	 2C	 22	 11	 64
	0.9 - 1.2	 0.01F	 0.05B	 0.14B	 2C	 22	 9	 64
	1.5 - 1.7	 0.01F	 0.045B	 0.14B	 2C	 24	 9	 62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.5 - 1.7

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B831	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded