Project Name:	TBL
	Project Code:	TBL	Site ID:	B840	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	B. Slater	Locality:
	Date Desc.:	19/02/87	Elevation:	No Data
	Map Ref.:	Sheet No. : 8843   1:100000	Rainfall:	0
	Northing/Long.:	149.983333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-29.15	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Vertic Calcic Grey Chromosol     	Principal Profile Form:	Dy2.33
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Chloris ventricosa
	Mid Strata - , , . *Species includes - Geijera parviflora, Eremophila mitchellii
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Casuarina cristata, Eucalyptus populnea, Acacia harpophylla
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); Brown (7.5YR4/2-Dry); ; Clay loam; Weak grade of 
	structure, 10-20 mm, Angular blocky; Massive grade of structure; Dry; Weak consistence; 0-
	2%, medium gravelly, 6-20mm, subrounded, Substrate material, coarse fragments; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 7.5 (pH meter); Clear change to - 
	A12	0.04 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Loam; Weak grade of structure, 10-20 mm, Angular 
	blocky; Massive grade of structure; Dry; Firm consistence; 0-2%, medium gravelly, 6-20mm, 
	subrounded, Substrate material, coarse fragments; Common (10 - 20 %), Ferromanganiferous, 
	Medium (2 -6 mm), Nodules; Clear change to - 
	A25B	0.1 - 0.15 m	Greyish brown (10YR5/2-Moist); White (10YR8/1-Dry); ; Clay loam; Weak grade of structure, 
	20-50 mm, Angular blocky; Weak grade of structure; Dry; Firm consistence; 0-2%, medium 
	gravelly, 6-20mm, subrounded, Substrate material, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules; Abrupt change to - 
	B21t	0.15 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Prismatic; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Strong consistence; 0-2%, medium gravelly, 6-20mm, subrounded, Substrate material, coarse 
	fragments; Few (2 - 10 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules; Gradual change to - 
	0.2 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Medium heavy clay; Moderate grade of structure, 50-100 
	mm, Subangular blocky; Smooth-ped fabric; Very strong consistence; 0-2%, medium gravelly, 
	6-20mm, subrounded, Substrate material, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), 
	Nodules; Field pH 9 (pH meter); Gradual change to - 
	B22t	0.3 - 0.44 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Moderate grade of structure, Lenticular; Smooth-
	ped fabric; Dry; Very strong consistence; 2-10%, medium gravelly, 6-20mm, subrounded, 
	Substrate material, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Fine (0 - 2 mm), 
	Nodules; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Gradual change to - 

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B840	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B23	0.44 - 0.6 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Moderate grade of structure, Lenticular; Smooth-
	ped fabric; Dry; Very strong consistence; 2-10%, medium gravelly, 6-20mm, subrounded, 
	Substrate material, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Fine (0 - 2 mm), 
	Nodules; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.9 (pH meter); 
	Gradual change to - 
	B24	0.6 - 0.9 m	Yellowish brown (10YR5/4-Moist); ; Medium heavy clay; Moderate grade of structure, 
	Lenticular; Smooth-ped fabric; Dry; Very strong consistence; 2-10%, medium gravelly, 6-20mm, 
	subrounded, Substrate material, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Fine 
	(0 - 2 mm), Nodules; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Nodules; Field pH 8.5 (pH 
	meter); Gradual change to - 
	B25	0.9 - 1.2 m	Pale brown (10YR6/3-Moist); ; Medium heavy clay; Moderate grade of structure, Lenticular; 
	Smooth-ped fabric; Dry; Very strong consistence; Few (2 - 10 %), Ferromanganiferous, Fine (0
	 - 2 mm), Nodules; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Nodules; Field pH 8.6 (pH 
	meter); Gradual change to - 
	B26	1.2 - 1.5 m	Light brownish grey (10YR6/2-Moist); ; Medium clay; Moderate grade of structure, Lenticular; 
	Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 
	mm), Nodules; Field pH 8.4 (pH meter); Gradual change to - 
	1.5 - 1.72 m	Light brownish grey (10YR6/2-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, 
	Lenticular; Smooth-ped fabric; Very strong consistence; Gradual change to - 
	Morphological Notes
	Observation Notes
	LAYERS RENUMBERED 12/10/92                                                                                              
	Site Notes
	TARA

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B840	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	8.2H	 0.06B	 20.4K	 2.9	 1.8	 0.1	 2.1D
	0.04 - 0.1	8.5H	 0.04B	 18.4K	 2.5	 0.9	<0.1	 2.7D
	0.1 - 0.15	8.7H	 0.06B	 17.2K	 5	 0.7	 0.2	 4.1D
	0.15 - 0.2	8.8H	 0.09B	 16.9K	 6.6	 0.4	 1.6	 2.9D
	0.2 - 0.3	8.8H	 0.17B
	0.44 - 0.6	8.8H	 0.35B	 10.7K	 9.9	 0.1	 5	 0.7D
	0.6 - 0.9	8.8H	 0.37B	 9.9K	 10.4	 0.2	 5.6	<0.1D
	0.9 - 1.2	8.4H	 0.37B	 8.3K	 10.9	 0.3	 6.6	 1.5D
	1.5 - 1.72	4.8H	 0.35B	 6.8K	 10	 0.2	 6.9	 7D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.63C	 2.57A	 105B	 0.057F	 0.272B	 0.31B	 24C	 33	 8	 27
	0.04 - 0.1	 0.34C	 1.37A	 27B	 0.036F	 0.144B	 0.24B	 23C	 35	 8	 31
	0.1 - 0.15	 0.36C	 0.84A	 11B	 0.025F	 0.104B	 0.23B	 22C	 31	 7	 37
	0.15 - 0.2	 4.49C	 0.67A	 10B	 0.023F	 0.078B	 0.21B	 20C	 27	 8	 39
	0.2 - 0.3	 8.82C	 0.52A	 6B	 0.017F	 0.062B	 0.17B	 20C	 25	 7	 38
	0.44 - 0.6	 2.19C	 0.01F	 0.026B	 0.15B	 20C	 28	 10	 40
	0.6 - 0.9	 1.71C	 0.01F	 0.029B	 0.14B	 21C	 29	 10	 38
	0.9 - 1.2	 0.46C	 0.008F	 0.021B	 0.13B	 20C	 27	 10	 43
	1.5 - 1.72	 0.008F	 0.024B	 0.13B	 16C	 25	 13	 48
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.44 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.5 - 1.72

	Project Name:	TBL
	Project Code:	TBL	Site ID:	B840	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded