Project Name:	WQA
	Project Code:	WQA	Site ID:	B604	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 90 metres
	Map Ref.:	Sheet No. : 6948   1:100000	Rainfall:	221
	Northing/Long.:	140.341666666667	Runoff:	Very rapid
	Easting/Lat.:	-24.6875	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Kw	Substrate Material:	Auger boring, No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Pediment
	10%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.43
	ASC Confidence:	Great Soil Group:	Desert loam
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, , Gravel
	Profile Morphology
	A1	0 - 0.1 m	Reddish yellow (5YR6/6-Dry); ; Fine sandy loam; Massive grade of structure; Dry; Weak 
	consistence; 2-10%, medium gravelly, 6-20mm, Gravel, coarse fragments; Field pH 6.7 (pH 
	meter); Clear change to - 
	A2	0.1 - 0.14 m	Pink (5YR7/4-Dry); ; Fine sandy loam; Massive grade of structure; Dry; Weak consistence; 2-
	10%, medium gravelly, 6-20mm, Gravel, coarse fragments; Field pH 7.1 (pH meter); Sharp 
	change to - 
	B2	0.14 - 0.2 m	Red (2.5YR4/6-Moist); Red (2.5YR5/6-Dry); ; Light medium clay; Strong grade of structure, 5-10
	 mm, Polyhedral; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Field 
	pH 7.1 (pH meter); Gradual change to - 
	B2	0.2 - 0.3 m	Red (2.5YR4/6-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Polyhedral; Dry; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Field pH 7.6 (pH meter); Gradual 
	change to - 
	B2	0.3 - 0.4 m	Yellowish red (5YR5/6-Moist); ; Light clay; , Polyhedral; Dry; Firm consistence; 2-10%, fine 
	gravelly, 2-6mm, coarse fragments; Field pH 8 (pH meter); Gradual change to - 
	0.4 - 0.6 m	Yellowish red (5YR5/6-Moist); ; Sandy loam; Weak consistence; 10-20%, medium gravelly, 6-
	20mm, coarse fragments; Field pH 8.3 (pH meter); Gradual change to - 
	0.6 - 0.9 m	Red (2.5YR5/6-Moist); ; Sandy loam; Weak consistence; 20-50%, medium gravelly, 6-20mm, 
	coarse fragments; Field pH 7.2 (pH meter); Gradual change to - 
	0.9 - 1.2 m	Red (2.5YR5/6-Moist); ; Sandy loam; Weak consistence; 20-50%, coarse fragments; Field pH 
	6.8 (pH meter); Gradual change to - 
	1.2 - 1.3 m	Red (2.5YR5/6-Moist); ; Sandy loam; Weak consistence; 20-50%, coarse fragments; Field pH 7 
	(pH meter); 
	Morphological Notes
	Observation Notes
	NO VEGETATION AT SITE.                                                                                                  
	Site Notes
	MONKIRA

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B604	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B604	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.7H	 0.014B
	0.1 - 0.14	7.1H	 0.018B
	0.14 - 0.2	7.1H	 0.039B
	0.2 - 0.3	7.6H	 0.051B
	0.3 - 0.4	8H	 0.059B
	0.4 - 0.6	8.3H	 0.21B
	0.6 - 0.9	7.2H	 1.5B
	0.9 - 1.2	6.8H	 1.4B
	1.2 - 1.3	7H	 0.62B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.14A	 20B	 0.033F	 0.02B	 0.71B	 7C	 62	 14	 16
	0.1 - 0.14	 0.05A	 0.013B	 9C	 51	 17	 23
	0.14 - 0.2	 4B	 0.033F	 0.93B
	0.2 - 0.3	 0.13A	 0.026B	 4C	 30	 23	 42
	0.3 - 0.4	 0.02C
	0.4 - 0.6	 0.29C	 0.12A	 0.025F	 0.011B	 0.78B	 56C	 28	 11	 4
	0.6 - 0.9
	0.9 - 1.2	 0.017F	 0.6B	 38C	 45	 9	 4
	1.2 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.14
	0.14 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.3

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B604	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction