Project Name:	WQA
	Project Code:	WQA	Site ID:	B619	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 140 metres
	Map Ref.:	Sheet No. : 7347   1:1000	Rainfall:	278
	Northing/Long.:	142.022222222222	Runoff:	Moderately rapid
	Easting/Lat.:	-25.3611111111111	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	   Q	Substrate Material:	Auger boring, 1 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Very severe (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Tall Strata - Shrub, 3.01-6m, Very sparse. *Species includes - Acacia aneura, Hakea species, Acacia species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Light red (2.5YR6/6-Dry); ; Sandy loam; Weak grade of structure, Platy; Massive grade of 
	structure; Dry; Weak consistence; Very few (0 - 2 %), Unidentified, Fine (0 - 2 mm), Nodules; 
	Field pH 6 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	B2	0.1 - 0.2 m	Red (2.5YR4/6-Moist); Red (2.5YR5/6-Dry); ; Sandy loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Weak consistence; Field pH 5.3 (pH meter); Gradual change to - 
	B2	0.2 - 0.3 m	Red (2.5YR4/6-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; Field pH 5.2 (pH meter); Gradual change to - 
	B2	0.3 - 0.6 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; Field pH 5.1 (pH meter); Gradual change to - 
	B2	0.6 - 0.9 m	Red (2.5YR4/6-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Dry;
	 Weak consistence; Field pH 5.1 (pH meter); Gradual change to - 
	0.9 - 1.2 m	Red (2.5YR4/8-Moist); Red (2.5YR5/8-Dry); ; Sandy clay loam (Light); Massive grade of 
	structure; Weak consistence; Field pH 5.2 (pH meter); Gradual change to - 
	1.2 - 1.35 m	Red (2.5YR4/8-Moist); Yellowish red (5YR5/8-Dry); ; Sandy clay loam (Heavy); Massive grade 
	of structure; Weak consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Field pH 5.2 (pH meter); Gradual change to - 
	1.35 - 1.5 m	Light red (2.5YR6/6-Moist); , 10YR76, 20-50% , 5-15mm, Distinct; , 10YR82, 20-50% , 5-15mm, 
	Distinct; Sandy clay loam; Massive grade of structure; Weak consistence; Few (2 - 10 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 5.3 (pH meter); Diffuse change to - 
	1.5 - 1.8 m	Light red (2.5YR6/6-Moist); , 10YR76, 20-50% , 5-15mm, Distinct; , 10YR82, 20-50% , 5-15mm, 
	Distinct; Sandy clay loam; Massive grade of structure; Weak consistence; 2-10%, medium 
	gravelly, 6-20mm, Gravel, coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), 
	Nodules; Field pH 5.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B619	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	CANT'BURY BORE

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B619	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6H	<0.01B
	0.1 - 0.2	5.3H	<0.01B
	0.2 - 0.3	5.2H	<0.01B
	0.3 - 0.6	5.1H	 0.01B
	0.6 - 0.9	5.1H	 0.01B
	0.9 - 1.2	5.2H	 0.01B
	1.2 - 1.35	5.2H	 0.01B
	1.35 - 1.5	5.3H	 0.01B
	1.5 - 1.8	5.8H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.31A	 24B	 0.025F	 0.03B	 0.37B	 34C	 45	 6	 15
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6	 0.12A	 0.021F	 0.023B	 0.41B	 30C	 41	 5	 25
	0.6 - 0.9
	0.9 - 1.2	 0.11A	 0.02F	 0.02B	 0.47B	 38C	 33	 6	 24
	1.2 - 1.35
	1.35 - 1.5
	1.5 - 1.8	 0.06A	 0.022F	 0.022B	 0.43B	 30C	 38	 4	 29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.35
	1.35 - 1.5
	1.5 - 1.8

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B619	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded