Project Name:	WQA
	Project Code:	WQA	Site ID:	B623	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 130 metres
	Map Ref.:	Sheet No. : 7447   1:100000	Rainfall:	278
	Northing/Long.:	142.763888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-25.3972222222222	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	No Data	Relief:	2 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endohypersodic Self-Mulching Brown Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, , Gravel
	Profile Morphology
	A1	0 - 0.05 m	Greyish brown (10YR5/2-Moist); Light brownish grey (10YR6/2-Dry); ; Medium heavy clay; 
	Strong grade of structure, 2-5 mm, Granular; Dry; Loose consistence; Clear change to - 
	B2	0.05 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Dry; Very firm consistence; 
	B2	0.1 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Dry; Very firm consistence; Gradual change to - 
	B2	0.2 - 0.3 m	Brown (10YR5/3-Moist); Pale brown (10YR6/3-Dry); ; Medium heavy clay; Strong grade of 
	structure, 20-50 mm, Angular blocky; Dry; Strong consistence; 
	B2	0.3 - 0.6 m	Brown (10YR5/3-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong consistence; 
	B2	0.6 - 0.9 m	Brown (10YR5/3-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong consistence; Very few 
	(0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Gypseous, , Crystals; 
	B2	0.9 - 1.2 m	Brown (10YR5/3-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong consistence; Very few 
	(0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Gypseous, , Crystals; 
	B2	1.2 - 1.5 m	Brown (10YR5/3-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong consistence; Very few 
	(0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Gypseous, , Crystals; 
	Diffuse change to - 
	B2	1.5 - 1.8 m	Light yellowish brown (10YR6/4-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong 
	consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), 
	Gypseous, , Crystals; 
	B2	1.8 - 2 m	Light yellowish brown (10YR6/4-Moist); ; Medium heavy clay; , Lenticular; Dry; Strong 
	consistence; 
	Morphological Notes
	Observation Notes
	SITE DEVOID OF VEGETATION AT TIME OF SAMPLING.                                                                          
	Site Notes
	WINDORAH

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B623	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B623	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.1H	 0.029B	 16K	 6	 1	 0.64	 3.4D
	0.05 - 0.1	7.2H	 0.037B	 17.8K	 6.1	 0.83	 1	 3.8D
	0.1 - 0.2	7.6H	 0.028B
	0.2 - 0.3	7.7H	 0.032B	 18.4K	 5.7	 0.68	 1.9	 1.8D
	0.3 - 0.6	7.8H	 0.11B
	0.6 - 0.9	8.1H	 0.28B
	0.9 - 1.2	8.3H	 0.4B
	1.2 - 1.5	7.8H	 1.2B
	1.5 - 1.8	7.5H	 0.73B
	1.8 - 2	7.3H	 0.54B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.27A	 84B	 0.035F	 0.045B	 0.71B	 7C	 34	 21	 39
	0.05 - 0.1	 0.19A	 86B	 0.03F	 0.021B	 0.67B	 6C	 29	 18	 46
	0.1 - 0.2	 0.15A
	0.2 - 0.3	 0.14A	 0.034F	 0.029B	 0.73B	 6C	 31	 21	 42
	0.3 - 0.6	 0.03C	 0.14A	 0.03F	 0.019B	 0.66B	 6C	 31	 20	 44
	0.6 - 0.9	 0.08C
	0.9 - 1.2	 0.16C	 0.09A	 0.044F	 0.014B	 0.81B	 4C	 29	 21	 45
	1.2 - 1.5	 0.06C
	1.5 - 1.8
	1.8 - 2	 0.06A	 0.041F	 0.014B	 0.81B	 3C	 32	 20	 45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B623	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction