Project Name:	WQA
	Project Code:	WQA	Site ID:	B639	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 245 metres
	Map Ref.:	Sheet No. : 7944   1:100000	Rainfall:	360
	Northing/Long.:	145.363888888889	Runoff:	Slow
	Easting/Lat.:	-26.8083333333334	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qr	Substrate Material:	Auger boring, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	Gn2.12
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Tall Strata - Tree, , Isolated plants. *Species includes - Acacia aneura, Eucalyptus populnea
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.1 m	Red (2.5YR5/6-Moist); ; Clay loam; Massive grade of structure; Weak consistence; 0-2%, fine 
	gravelly, 2-6mm, Substrate material, coarse fragments; 
	0.1 - 0.2 m	Red (2.5YR4/6-Moist); ; Clay loam (Heavy); Massive grade of structure; Weak consistence; 0-
	2%, fine gravelly, 2-6mm, Substrate material, coarse fragments; 
	0.2 - 0.3 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Weak consistence; 0-2%, fine 
	gravelly, 2-6mm, Substrate material, coarse fragments; 
	0.3 - 0.6 m	Red (2.5YR5/8-Moist); ; Light clay; Massive grade of structure; Weak consistence; 2-10%, 
	medium gravelly, 6-20mm, Substrate material, coarse fragments; 
	0.6 - 0.8 m	Red (2.5YR5/8-Moist); ; Light clay; Massive grade of structure; Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, Substrate material, coarse fragments; Clear change to - 
	0.8 - 0.9 m	Red (2.5YR5/8-Moist); , 10YR66, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Light 
	medium clay; Massive grade of structure; Weak consistence; 2-10%, fine gravelly, 2-6mm, 
	Substrate material, coarse fragments; 
	0.9 - 1.05 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Weak grade of structure, Polyhedral; Firm 
	consistence; 10-20%, fine gravelly, 2-6mm, Substrate material, coarse fragments; 
	1.05 - 1.13 m	White (10YR8/1-Moist); , 2.5Y76, 20-50% , 0-5mm, Prominent; , 20-50% , 0-5mm, Prominent; 
	Massive grade of structure; Very firm consistence; 20-50%, fine gravelly, 2-6mm, Substrate 
	material, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	YARRONVALE

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B639	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9H	 0.011B	 1.8K	 0.77	 0.8	 0.09	 6.2D
	0.1 - 0.2	4.9H	 0.011B
	0.2 - 0.3	5.1H	 0.01B
	0.3 - 0.6	5.7H	 0.024B	 2.9K	 1.4	 0.46	 0.1	 3D
	0.6 - 0.8	6.3H	 0.009B
	0.8 - 0.9	6.9H	 0.011B
	0.9 - 1.05	7.6H	 0.018B	 5.2K	 5	 0.58	 0.39	 1.9D
	1.05 - 1.13	7.5H	 0.029B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.47A	 4B	 0.032F	 0.046B	 0.44B	 14C	 40	 12	 34
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6	 0.15A	 0.022F	 0.03B	 0.45B	 10C	 40	 12	 36
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.05	 0.1A	 0.02F	 0.021B	 0.46B	 5C	 31	 12	 54
	1.05 - 1.13	 0.11A	 0.015F	 0.022B	 0.44B	 23C	 29	 15	 31
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1.05
	1.05 - 1.13

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B639	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction