Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A49	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.B. Wells	Locality:
	Date Desc.:	24/05/54	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-9   1:250000	Rainfall:	0
	Northing/Long.:	138.925	Runoff:	Moderately rapid
	Easting/Lat.:	-34.5144444444445	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mesonatric Grey Sodosol     	Principal Profile Form:	Dd1.13
	ASC Confidence:	Great Soil Group:	Solodized 
	Analytical data are incomplete but reasonable confidence.	solonetz
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.11 m	Greyish brown (10YR5/2-Moist); Light brownish grey (10YR6/2-Dry); ; Loamy fine sand; 5-10 
	mm, Granular; Strong consistence; Field pH 7 (pH meter); 
	B1	0.11 - 0.22 m	Very dark grey (10YR3/1-Moist); ; Sandy medium clay; Strong grade of structure, 20-50 mm, 
	Prismatic; Strong consistence; Moderately plastic; Field pH 8 (pH meter); Gradual change to - 
	B1	0.22 - 0.38 m	Grey (10YR5/1-Moist); ; Medium clay; Strong grade of structure, 100-200 mm, Prismatic; Strong 
	grade of structure, 20-50 mm, Angular blocky; Strong consistence; Moderately plastic; Field pH 
	8.5 (pH meter); Gradual change to - 
	B2	0.38 - 0.51 m	; Medium clay; Strong grade of structure, 100-200 mm, Prismatic; Strong grade of structure, 20-
	50 mm, Angular blocky; Strong consistence; Moderately plastic; Few (2 - 10 %), Calcareous, , 
	Soft segregations; Field pH 9 (pH meter); Gradual change to - 
	Bk	0.51 - 0.66 m	; Medium clay; Strong grade of structure, 100-200 mm, Prismatic; Strong grade of structure, 20-
	50 mm, Angular blocky; Strong consistence; Moderately plastic; Few (2 - 10 %), Calcareous, , 
	Soft segregations; Field pH 9 (pH meter); Diffuse change to - 
	BC	0.66 - 0.79 m	; Medium clay; Strong grade of structure, 100-200 mm, Prismatic; Strong grade of structure, 20-
	50 mm, Angular blocky; Strong consistence; Moderately plastic; Very few (0 - 2 %), 
	Calcareous, , Soft segregations; Field pH 9 (pH meter); Diffuse change to - 
	C	1.67 - 1.98 m	; Medium clay; Moderately plastic; Field pH 7.5 (pH meter); 
	Morphological Notes
	Observation Notes
	SUBSTRATE MATERIAL - SILICA                                                                                             
	Site Notes
	BAROSSA LIGHT

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A49	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	7.4A	 0.088C
	0.11 - 0.22	8.2A	 0.097C	 5.3F	 6.4	 0.88	 3.1	 1.3E
	0.22 - 0.38	8.9A	 0.2C
	0.38 - 0.51	9.4A	 0.26C
	0.51 - 0.66	9.6A	 0.26C
	0.66 - 0.79	9.6A	 0.26C
	1.67 - 1.98	9A	 0.26C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	 1	 22C	 55	 8	 13
	0.11 - 0.22	 0.01A	 19C	 35	 6	 37
	0.22 - 0.38	 0.04A	 14C	 28	 9	 47
	0.38 - 0.51	 4.8A	 10C	 25	 14	 45
	0.51 - 0.66	 4.4A	 6C	 23	 17	 49
	0.66 - 0.79	 1.3A	 5C	 25	 21	 45
	1.67 - 1.98	 0.02A	 2C	 42	 20	 36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.11 - 0.22
	0.22 - 0.38
	0.38 - 0.51
	0.51 - 0.66
	0.66 - 0.79
	1.67 - 1.98

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A49	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded