Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.B. Wells	Locality:	PRIMARILY VITICULTURE WHERE CLEARED: 
	WATERLOGGING IN LOWER LYING AREAS:
	Date Desc.:	25/05/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.919166666667	Runoff:	Moderately rapid
	Easting/Lat.:	-34.5733333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Yellow Sodosol     	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	Solodized 
	Analytical data are incomplete but reasonable confidence.	solonetz
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus leucoxylon, Astrebla species
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.14 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Field pH 6.5 (pH meter); Gradual change to - 
	A1	0.14 - 0.27 m	Pale brown (10YR6/3-Moist); ; Sand; Single grain grade of structure; Loose consistence; Field 
	pH 6.5 (pH meter); Gradual change to - 
	A2	0.32 - 0.47 m	White (10YR8/2-Moist); ; Sand; Single grain grade of structure; Loose consistence; Field pH 6.5 
	(pH meter); Sharp change to - 
	B1	0.47 - 0.57 m	Brownish yellow (10YR6/8-Moist); , 10YR62; , 10YR74; Sandy medium clay; 20-50 mm, 
	Prismatic; Moderately plastic; Field pH 6 (pH meter); 
	B2	0.57 - 0.74 m	; Sandy medium clay; Massive grade of structure, Columnar; Firm consistence; Field pH 8 (pH 
	meter); Abrupt change to - 
	B2	0.74 - 0.81 m	; Sandy medium clay; Strong grade of structure; Firm consistence; Field pH 6.5 (pH meter); 
	BC	0.81 - 0.99 m	; Sandy medium clay; 50-100 mm, Prismatic; Very firm consistence; Field pH 8 (pH meter); 
	Gradual change to - 
	Bk	0.99 - 1.12 m	; Sandy medium clay; Massive grade of structure; Very firm consistence; 2-10%, rounded, 
	Quartz, coarse fragments; Field pH 8.3 (pH meter); 
	C	1.78 - 1.88 m	; Sandy medium clay; Very strong consistence; 10-20%, rounded, Quartz, coarse fragments; 
	Field pH 8.4 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BAROSSA LIGHT

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	6.7A	 0.009C	 1.9F	 0.4	 0.15	 0.08	 1.3E
	0.14 - 0.27	6.9A	 0.007C
	0.32 - 0.47	6.8A	 0.005C
	0.47 - 0.57	6.3A	 0.039C	 3.7F	 6.8	 0.27	 2.3	 6.3E
	0.57 - 0.74	7.1A	 0.057C	 3.2F	 5.6	 0.22	 2.2	 3.4E
	0.74 - 0.81	6.6D	 0.088C	 5.8F	 10.4	 0.41	 4	 7.7E
	0.81 - 0.99	8.1A	 0.13C
	0.99 - 1.12	9.3A	 0.23C
	1.78 - 1.88	9.1A	 0.36C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	 0.037C	 49C	 45	 4	 1
	0.14 - 0.27
	0.32 - 0.47
	0.47 - 0.57	 0.038C	 29C	 23	 1	 46
	0.57 - 0.74	 6	 40C	 27	 0	 35
	0.74 - 0.81	 22C	 14	 0	 65
	0.81 - 0.99	 0.02A
	0.99 - 1.12	 1A
	1.78 - 1.88	 15A	 1	 20C	 23	 1	 42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.14
	0.14 - 0.27
	0.32 - 0.47
	0.47 - 0.57
	0.57 - 0.74
	0.74 - 0.81
	0.81 - 0.99
	0.99 - 1.12
	1.78 - 1.88

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	5_C_B	Water soluble Chloride - Method recorded as B
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded