Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:	CEREAL + PEA CROPPING: VOLUNTEER PASTURE:
	Date Desc.:	27/05/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.910555555556	Runoff:	Rapid
	Easting/Lat.:	-34.5252777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-32%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Red Sodosol     	Principal Profile Form:	Db2.13
	ASC Confidence:	Great Soil Group:	Brown earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus obliqua
	Surface Coarse Fragments:
	Profile Morphology
	AB	0 - 0.22 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Moderate grade of structure, Granular; 
	Weak grade of structure, 50-100 mm, Angular blocky; Strong consistence; Field pH 6.5 (pH 
	meter); , fine (1-2mm) roots; Sharp, Irregular change to - 
	B	0.22 - 0.53 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Angular blocky; Strong grade of structure, 200-500 mm, Prismatic; Coarse, (10 - 20) mm crack; 
	Strong consistence; Field pH 7.5 (pH meter); , fine (1-2mm) roots; Abrupt, Irregular change to - 
	B	0.53 - 0.84 m	Yellowish red (5YR4/7-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Prismatic;
	 Fine, (0 - 5) mm crack; Very strong consistence; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Field pH 8.4 (pH meter); 
	C	1.37 - 1.83 m	Yellowish red (5YR4/7-Moist); ; Medium clay; Rigid consistence; Few (2 - 10 %), Calcareous, , 
	Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	BAROSSA LIGHT

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.22	7.6A	 0.022C	 15
	0.22 - 0.53	8A	 0.045C	 30
	0.53 - 0.84	9.2A	 0.091C
	1.37 - 1.83	8.9A	 0.37C	 8.3F	 15.3	 1.5	 8.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.22	 0.015F	 0.095A	 1	 3C	 43	 15	 35
	0.22 - 0.53	 0.05A	 0.016F	 0.099A
	0.53 - 0.84	 30A
	1.37 - 1.83	 0.04A	 4	 1C	 21	 15	 62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.22
	0.22 - 0.53
	0.53 - 0.84
	1.37 - 1.83

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded