Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.B. Wells	Locality:	CEREAL + PEA CROPS: VOLUNTEER PASTURE FOR 
	GRAZING:
	Date Desc.:	28/05/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.910555555556	Runoff:	Rapid
	Easting/Lat.:	-34.5258333333334	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-32%	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic-Vertic Pedal Calcic Calcarosol     	Principal Profile Form:	Uf6.11
	ASC Confidence:	Great Soil Group:	Rendzina
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus obliqua
	Surface Coarse Fragments:
	Profile Morphology
	AB	0 - 0.09 m	Dark reddish brown (5YR2/3-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Granular; Very firm consistence; Field pH 8.3 (pH meter); Clear change to - 
	B1	0.09 - 0.23 m	Dark reddish brown (5YR2/2-Moist); ; Medium clay; 2-5 mm, Granular; Weak grade of structure, 
	20-50 mm, Angular blocky; Very weak consistence; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Field pH 8.3 (pH meter); Gradual change to - 
	B	0.3 - 0.41 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; , Granular; Very weak consistence; Few 
	(2 - 10 %), Calcareous, , Soft segregations; Field pH 8.3 (pH meter); Gradual change to - 
	B3	0.41 - 0.64 m	; Medium clay; , Granular; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft 
	segregations; Field pH 8.3 (pH meter); Gradual change to - 
	0.64 - 0.81 m	; Medium clay; , Granular; Very weak consistence; 
	Morphological Notes
	Observation Notes
	64-81CM HIGHLY CALCAREOUS:                                                                                              
	Site Notes
	BAROSSA LIGHT

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	7.7A	 0.031C	 20.4F	 3.5	 1.7	 0.24	 3.8E
	0.09 - 0.23	8.4A	 0.052C
	0.3 - 0.41	8.7A	 0.047C
	0.41 - 0.64	8.7A	 0.046C
	0.64 - 0.81	8.8A	 0.044C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	 0.05A	 0.024F	 0.15C	 1B	 2	 3C	 43	 19	 31
	0.09 - 0.23	 3.6A	 0.024F	 0.16A	 1B	 1	 2C	 37	 15	 39
	0.3 - 0.41	 26A
	0.41 - 0.64	 14A	 1	 1C	 33	 12	 37
	0.64 - 0.81	 27A	 1C	 28	 8	 34
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.23
	0.3 - 0.41
	0.41 - 0.64
	0.64 - 0.81

	Project Name:	Barossa Valley II, S.A.
	Project Code:	BA1	Site ID:	A62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	17A_NR	Total element - K(%) - Not recorded
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded