Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	VINEYARD:
	Date Desc.:	21/06/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.856944444444	Runoff:	Rapid
	Easting/Lat.:	-34.5708333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Flood plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	Red-brown earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Brown (7.5YR4/2-Moist); ; Loamy sand; Single grain grade of structure; Moist; Weak 
	consistence; Field pH 6.5 (pH meter); Diffuse change to - 
	A2	0.18 - 0.3 m	; Sand; Single grain grade of structure; Field pH 6 (pH meter); Clear, Irregular change to - 
	B1	0.3 - 0.38 m	Reddish brown (2.5YR4/4-Moist); , 10YR44; Medium clay; , Angular blocky; , Prismatic; Weak 
	consistence; Field pH 6 (pH meter); Many, fine (1-2mm) roots; Diffuse change to - 
	B2	0.38 - 0.56 m	; Medium clay; , Angular blocky; , Prismatic; Moist; Weak consistence; Field pH 6 (pH meter); 
	Many, fine (1-2mm) roots; Diffuse change to - 
	B3	0.56 - 0.76 m	; , Prismatic; Strong consistence; Field pH 6 (pH meter); Many, fine (1-2mm) roots; Diffuse 
	change to - 
	B	0.84 - 0.97 m	; 20-50 mm, Prismatic; Strong consistence; Field pH 8.3 (pH meter); 
	B	0.97 - 1.42 m	; Strong consistence; 
	1.68 - 1.75 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	LIGHT

	Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.6A	 0.011C	 3.3F	 0.4	 0.46	 0.17	 2.3E
	0.18 - 0.3	6.7A	 0.01C
	0.3 - 0.38	6.6A	 0.021C
	0.38 - 0.56	6.8A	 0.033C
	0.56 - 0.76	7.6A	 0.03C	 12.6F	 7.1	 1.2	 0.83	 3.6E
	0.84 - 0.97	8.6A	 0.054C
	0.97 - 1.42	8.8A	 0.061C
	1.68 - 1.75
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.018F	 0.041C	 2B	 12	 32C	 55	 7	 6
	0.18 - 0.3
	0.3 - 0.38	 0.058A	 2	 21C	 25	 0	 55
	0.38 - 0.56	 1	 15C	 15	 1	 70
	0.56 - 0.76	 0.012F	 2B	 1	 18C	 27	 0	 54
	0.84 - 0.97	 3.1A
	0.97 - 1.42	 6.5A
	1.68 - 1.75
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.18 - 0.3
	0.3 - 0.38
	0.38 - 0.56
	0.56 - 0.76
	0.84 - 0.97
	0.97 - 1.42
	1.68 - 1.75

	Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	17A_NR	Total element - K(%) - Not recorded
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded