Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A66	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	VOLUNTEER PASTURE + SOME CROPPING + SOME 
	HORTICULTURE:
	Date Desc.:	23/06/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.867777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-34.54	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.33
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus odorata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.11 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Single grain grade of structure; Very firm 
	consistence; Field pH 6 (pH meter); Clear, Irregular change to - 
	B1	0.13 - 0.33 m	Dark red (2.5YR3/6-Moist); , 5YR46; Medium clay; 20-50 mm, Angular blocky; 5-10 mm, 
	Prismatic; Firm consistence; Field pH 6.5 (pH meter); Gradual change to - 
	B12	0.33 - 0.46 m	Dark red (2.5YR3/6-Moist); , 5YR46; Sandy medium clay; 20-50 mm, Angular blocky; 5-10 mm, 
	Prismatic; Firm consistence; Field pH 7 (pH meter); Clear, Irregular change to - 
	B	0.48 - 0.58 m	; Sandy medium clay; Massive grade of structure; Very firm consistence; Field pH 8.3 (pH 
	0.84 - 1.02 m	; Sandy clay loam; Massive grade of structure; Strong consistence; 
	1.52 - 1.6 m	; Sandy clay loam; Massive grade of structure; Strong consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	BAROSSA LIGHT

	Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A66	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	6.6A	 0.015C	 2.8	 2.6E
	0.13 - 0.33	7.2A	 0.021C	 22.3F	 4.4	 18.2	 0.45	 5.7E
	 1.3
	0.33 - 0.46	7.6A	 0.023C	 21.9F	 4.1	 1.2	 0.49	 4.1E
	0.48 - 0.58	8.7A	 0.05C
	0.84 - 1.02	8.9A	 0.036C
	1.52 - 1.6	8.9A	 0.039C	 7.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	 0.012F	 0.057C	 1	 28C	 58	 8	 7
	0.13 - 0.33	 0.013F	 0.082C	 13C	 23	 2	 62
	0.33 - 0.46	 16C	 26	 2	 56
	0.48 - 0.58	 13A
	0.84 - 1.02	 6.6A	 5	 36C	 33	 2	 22
	1.52 - 1.6	 5.7A	 0.006F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.13 - 0.33
	0.33 - 0.46
	0.48 - 0.58
	0.84 - 1.02
	1.52 - 1.6

	Project Name:	Barossa Valley III, S.A.
	Project Code:	BA3	Site ID:	A66	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded