Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	GRAZING FOR DAIRY FARMING: SUB-CLOVER 
	ANNUAL GRASSES: UP TO 2 - 3 SHEEP PER ACRE
	Date Desc.:	05/10/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	139.071388888889	Runoff:	Slow
	Easting/Lat.:	-34.6966666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Calcic Grey Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized 
	No analytical data are available but confidence is fair.	solonetz
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	; Sandy loam; Weak consistence; Diffuse change to - 
	A12	0.05 - 0.19 m	; Sand (Heavy); Single grain grade of structure; Clear, Irregular change to - 
	A2	0.25 - 0.46 m	; Sand; Single grain grade of structure; Loose consistence; Clear, Irregular change to - 
	B1	0.46 - 0.51 m	; Sandy medium clay; 20-50 mm, Angular blocky; Weak grade of structure, Columnar; Gradual 
	change to - 
	B1	0.51 - 0.71 m	; Medium clay; 50-100 mm, Angular blocky; Diffuse change to - 
	B	0.71 - 0.89 m	; Sandy medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	B	1.24 - 1.32 m	; Sandy medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	STURT

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.7A	 0.062C	 8.3F	 2.5	 5.2	 1.1	 4.6E
	 0.42	 1.4
	0.05 - 0.19	7.5A	 0.042C
	0.25 - 0.46	8.1A	 0.041C	 1.2F	 0.9	 0.09	 0.35	 0.2E
	0.46 - 0.51	8.5A	 0.13C
	0.51 - 0.71	8.7A	 0.19C	 10.5F	 12.9	 32	 9.6
	 0.86	 1.5
	0.71 - 0.89	9.2A	 0.15C
	1.24 - 1.32	8.9A	 0.13C	 0.4	 1.6
	 20	 3.9
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.032F	 0.299C	 20C	 58	 16	 5
	0.05 - 0.19
	0.25 - 0.46	 0.01A	 25C	 59	 10	 5
	0.46 - 0.51	 0.03A
	0.51 - 0.71	 0.06A	 0.02F	 0.063C	 6C	 20	 10	 64
	0.71 - 0.89	 6.8A
	1.24 - 1.32	 1.1A	 0.019F	 1	 17C	 46	 6	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.19
	0.25 - 0.46
	0.46 - 0.51
	0.51 - 0.71
	0.71 - 0.89
	1.24 - 1.32

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction