Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	GRAZING: SUB-CLOVER: VOLUNTEER GRASSES & 
	WEEDS: 1 1/2 - 2 SHEEP PER ACRE
	Date Desc.:	06/10/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 6728   1:100000	Rainfall:	0
	Northing/Long.:	139.108611111111	Runoff:	Rapid
	Easting/Lat.:	-34.7133333333333	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	8 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Subnatric Black Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus leucoxylon
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Fibric); Single grain grade of structure; 
	CommonClear change to - 
	A12	0.08 - 0.18 m	Brown (10YR4/3-Moist); ; Sand; Massive grade of structure; Very firm consistence; 2-10%, 
	coarse gravelly, 20-60mm, Gravel, coarse fragments; ManyDiffuse change to - 
	A2	0.18 - 0.25 m	Greyish brown (10YR5/2-Moist); ; Sand; Massive grade of structure; Very firm consistence; 
	20-50%, cobbly, 60-200mm, Gravel, coarse fragments; CommonDiffuse change to - 
	B1	0.25 - 0.42 m	Very dark brown (10YR2/2-Moist); , 10R48; Medium clay; 10-20 mm, Angular blocky; Weak 
	grade of structure, Columnar; Very firm consistence; Clear change to - 
	B2	0.42 - 0.61 m	Very dark brown (10YR2/2-Moist); , 10R33; , 10R48; Sandy medium clay; Massive grade of 
	structure, Angular blocky; Strong consistence; 
	BC	0.61 - 0.91 m	; Sandy medium clay; 
	C	1.07 - 1.29 m	; 
	C	1.29 - 1.45 m	; 
	Morphological Notes
	Observation Notes
	107 - 145 CM HIGHLY MICACEOUS                                                                                           
	Site Notes

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6A	 0.023C	 4.4F	 1.1	 4.6	 0.2	 5.1E
	 0.32	 0.1
	0.08 - 0.18	5.8A	 0.007C
	0.18 - 0.25	6.1A	 0.009C
	0.25 - 0.42	6.5A	 0.008C	 3.6F	 2.8	 15	 0.6	 3.7E
	 0.32	 0.15
	0.42 - 0.61	6.9A	 0.011C	 3.4F	 3.2	 0.42	 0.46	 3.7E
	0.61 - 0.91	7.3A	 0.018C
	1.07 - 1.29	7.6A	 0.017C
	1.29 - 1.45	7.6A	 0.014C	 2.6F	 3.6	 48	 1.3	 0.5E
	 0.11	 0.76
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.015F	 0.179C	 1	 27C	 58	 9	 6
	0.08 - 0.18
	0.18 - 0.25
	0.25 - 0.42	 0.01F	 0.049C	 2	 14C	 42	 8	 34
	0.42 - 0.61	 2	 14C	 37	 7	 40
	0.61 - 0.91
	1.07 - 1.29
	1.29 - 1.45	 0.007F	 0.007C	 9C	 73	 7	 11
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.08 - 0.18
	0.18 - 0.25
	0.25 - 0.42
	0.42 - 0.61
	0.61 - 0.91
	1.07 - 1.29
	1.29 - 1.45

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction