Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	103A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	10/10/96	Elevation:	13 metres
	Map Ref.:	Sheet No. : 4966-1   1:50000	Rainfall:	No Data
	Northing/Long.:	8288219 AMG zone: 52	Runoff:	No runoff
	Easting/Lat.:	652950  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czs	Substrate Material:	Alluvium 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	52
	Haplic Self-Mulching Grey Vertosol Slightly gravelly Very fine 	Principal Profile Form:	UG5-24
	Very fine  Very deep
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Chrysopogon fallax, Ophiurous exaltatus
	Mid Strata - Shrub, 0.51-1m, Very sparse. *Species includes - Carissa lanceolata, Atalaya hemiglauca, Ophiurous exaltatus
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Lysiphyllum cunninghamii, Terminalia volucris
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Weak red (2.5YR4/2-Moist); , 0-0% ; Medium heavy clay; Strong grade of structure, <2 mm, 
	Granular; Rough-ped fabric; Medium, (5 - 10) mm crack; Common (1-5 per 100mm2)  
	macropores, Dry; Very plastic; Normal plasticity; Very sticky; Many cutans, >50% of ped faces 
	or walls coated, distinct; Few (2 - 10 %), Ferromanganiferous, , ; Field pH 7.5 (Raupach); Few, 
	medium (2-5mm) roots; Abrupt change to - 
	B2	0.02 - 1.2 m	Weak red (2.5YR4/2-Moist); , 0-0% ; Medium heavy clay; Strong grade of structure, 10-20 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; 
	Fine, (0 - 5) mm crack; Few (<1 per 100mm2)  macropores, Moderately moist; Very plastic; 
	Normal plasticity; Very sticky; Many cutans, >50% of ped faces or walls coated, distinct; Few 
	(2 - 10 %), Ferromanganiferous, , ; Field pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	PHOTO NO; SURFACE - 15, PROFILE - 14, OPEN WOODLAND (10% COVER), DOM LYSIPHYLLUM CUNNINGHANII, TERMINALIA 
	VOLUENS, OPHIUROHS EXALTATUS GUMS: CHRYSOPAGIN FALLAX, ATALAYA HEMIGLAUCA, RAINED 4 DAYS AGO, 
	CARRISA LANCEOLATA - SLIGHTLY ........

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	103A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.7C	0.07A
	7.1A
	0.1 - 0.2	7.2C	0.05A
	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.1 - 0.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.1 - 0.2

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	103A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1