Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	106A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/10/96	Elevation:	8 metres
	Map Ref.:	Sheet No. : 4966-1   1:50000	Rainfall:	No Data
	Northing/Long.:	8296620 AMG zone: 52	Runoff:	No runoff
	Easting/Lat.:	654599  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czs	Substrate Material:	Slightly porous, Alluvium 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Hardsetting, Cryptogam surface
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	12
	Episodic-Epicalcareous Crusty Brown Vertosol Non-gravelly 	Principal Profile Form:	N/A
	Medium fine Medium fine  Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida latifolia, Chrysopogon fallax
	Mid Strata - Shrub, 1.01-3m, Very sparse. *Species includes - Carissa lanceolata
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus microtheca, Excoecaria parvifolia, Lysiphyllum 
	cunninghamii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Dark yellowish brown (10YR4/6-Moist); ; Medium clay; Massive grade of structure; Earthy 
	fabric; Dry; Very plastic; Normal plasticity; Very sticky; 0-2%, medium gravelly, 6-20mm, 
	subrounded, dispersed, Sandstone, coarse fragments; Field pH 8 (Raupach); Few, very fine 
	(0-1mm) roots; Abrupt, Smooth change to - 
	B21	0.03 - 0.5 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Very plastic; Normal plasticity; Very 
	sticky; Field pH 7.5 (Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B2	0.5 -  m	Dark yellowish brown (10YR4/4-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 
	mm, Angular blocky; Smooth-ped fabric; Moderately moist; Very plastic; Normal plasticity; Very 
	sticky; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Concretions; Field pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	SIMILAR K104 BUT NOT.....
	Site Notes
	PHOTO NO; SURFACE 21  OPEN WOODLAND - : TREE- EUCALYPTUS MICROTHEEA, EXOCAERIA PARVIFLORA, LYSIPHYLLUM
	 CUNNINGHAMIL, CARISSA LANCEOLATA - SHRUB, ARISTIDA LATIFOLIA, CHRYSOPOGON FALLAX - GRASSES....

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	106A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.6C	0.04A
	6.2A
	0.1 - 0.2	4.9C	0.08A	3.76C	6.19	0.35	0.32	14.6K	10.6D	2.19
	5.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.1 - 0.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.1 - 0.2

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	106A	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15B1_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1