Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	02/09/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 4967   1:100000	Rainfall:	No Data
	Northing/Long.:	8295397 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	653292  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czs	Substrate Material:	Auger boring, 0.6 m deep,Slightly porous, 
	Colluvium 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Hardsetting, Cryptogam surface
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	52
	Endocalcareous-Endohypersodic Massive Brown Vertosol 	Principal Profile Form:	N/A
	Slightly gravelly Fine Medium fine  Deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	50-90%, cobbly, 60-200mm, subangular, Limestone
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); , 7.5YR58, 2-10% , 5-15mm, Faint; Light clay; Massive grade of 
	structure; Earthy fabric; Medium, (5 - 10) mm crack; Dry; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Concretions; Soil matrix is Slightly calcareous; Field pH 6 
	B1	0.1 - 0.3 m	Brown (7.5YR4/4-Moist); , 7.5YR58, 0-2% , 0-5mm, Faint; Light clay; Massive grade of 
	structure; Earthy fabric; Medium, (5 - 10) mm crack; Dry; Soil matrix is Slightly calcareous; Field 
	pH 6 (Raupach); 
	B12	0.3 - 0.6 m	Brown (10YR4/3-Moist); , 7.5YR58, 20-50% , 5-15mm, Prominent; Light medium clay; Moderate 
	grade of structure, 2-5 mm, Subangular blocky; Moderate grade of structure, 5-10 mm, 
	Lenticular; Smooth-ped fabric; Dry; 50-90%, cobbly, 60-200mm, subangular, dispersed, 
	Limestone, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; 
	Few (2 - 10 %), Ferromanganiferous, Extremely coarse (> 60 mm), Concretions; Soil matrix is 
	Slightly calcareous; Field pH 6 (Raupach); 
	BC	0.6 - 1 m	Brown (10YR4/3-Moist); , 7.5YR58, 0-2% , 5-15mm, Faint; Medium clay; Moderate grade of 
	structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; 50-90%, cobbly, 60-200mm, 
	subangular, dispersed, Limestone, coarse fragments; Common cutans, 10-50% of ped faces or
	 walls coated, distinct; Few (2 - 10 %), Ferromanganiferous, Extremely coarse (> 60 mm), 
	Concretions; Soil matrix is Slightly calcareous; Field pH 6 (Raupach); 
	C	1 - 1.4 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Moderate grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; 0-2%, cobbly, 60-200mm, subangular, dispersed, 
	Limestone, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), 
	Concretions; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Concretions; Soil matrix is 
	Slightly calcareous; Field pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	Deep brown mottled cracking clay, stopped at 140 cm by calcrete
	Site Notes

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile