Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	17/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 5067-3   1:50000	Rainfall:	No Data
	Northing/Long.:	8305330 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	687015  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Paj	Substrate Material:	Porous, Alluvium 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	76
	Bleached-Mottled Mesotrophic Grey Chromosol Thick Non-	Principal Profile Form:	N/A
	gravelly Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Fine sandy loam; Earthy fabric; Common (1-5 per 100mm2) 
	Very fine (0.075-1mm) macropores, Dry; Slightly plastic; Normal plasticity; Non-sticky; Field pH 
	5.5 (Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	A21e	0.1 - 0.3 m	Brown (10YR5/3-Moist); Light grey (10YR7/2-Dry); , 10YR56, 2-10% , 0-5mm, Distinct; Sandy 
	loam; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Non-plastic; Non-sticky; Field pH 5.5 (Raupach); Few, very fine (0-
	1mm) roots; Clear, Smooth change to - 
	A22e	0.3 - 0.6 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Smooth-ped 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-
	sticky; Field pH 5.5 (Raupach); Clear, Smooth change to - 
	A3j	0.6 - 0.7 m	Light brownish grey (10YR6/2-Moist); , 2.5YR36, 2-10% , 5-15mm, Distinct; Sandy loam; 
	Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moderately moist; Moderately plastic; Normal plasticity; Slightly sticky; Field pH 6 
	(Raupach); Clear, Smooth change to - 
	B2	0.7 - 0.9 m	Light brownish grey (10YR6/2-Moist); , 2.5YR36, 10-20% , 5-15mm, Distinct; , 7.5YR56; Light 
	clay; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Moderately moist; Very plastic; Normal plasticity; Moderately sticky; 0-2%, 
	medium gravelly, 6-20mm, rounded, stratified, Sandstone, coarse fragments; Field pH 6 
	(Raupach); 
	B3	0.9 - 1.1 m	Red (2.5YR4/6-Moist); , 10YR81, 10-20% , 5-15mm, Distinct; Sandy loam; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moderately moist; Very plastic; Normal plasticity; Moderately sticky; Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	PHOTO NO; SURFACE - 17,15,16, CATORACTS.  E.POLYCARPA.  ........

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile