Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	18/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 5067-4   1:50000	Rainfall:	No Data
	Northing/Long.:	8333672 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	668930  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Paa	Substrate Material:	Auger boring, Porous, Alluvium 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Surface crust, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	34
	Palic Regolithic Leptic Tenosol Medium Non-gravelly Loamy 	Principal Profile Form:	N/A
	Loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra, Chrysopogon fallax, Plectrachne 
	pungens	Mid Strata - Shrub, 1.01-3m, Mid-dense. *Species includes - Carissa lanceolata, Terminalia volucris
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus polycarpa
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, rounded, Sandstone
	Profile Morphology
	A11	0 - 0.1 m	Brown (7.5YR4/2-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-sticky; 0-
	2%, fine gravelly, 2-6mm, angular tabular, Siltstone, coarse fragments; Field pH 7 (Raupach); 
	Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	A12	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); Light brown (7.5YR6/4-Dry); , 0-0% ; Sandy loam (Light); Massive 
	grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Non-plastic; Non-sticky; 0-2%, fine gravelly, 2-6mm, angular tabular, 
	dispersed, Siltstone, coarse fragments; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; 
	B1	0.2 - 0.3 m	Yellowish red (5YR5/6-Moist); , 0-0% ; Sandy loam (Light); Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-sticky;
	 0-2%, fine gravelly, 2-6mm, angular tabular, Siltstone, coarse fragments; Field pH 7 (Raupach); 
	Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B2	0.3 - 1 m	Yellowish red (5YR5/8-Moist); , 0-0% ; Fine sandy loam; Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-sticky;
	 0-2%, fine gravelly, 2-6mm, angular tabular, Siltstone, coarse fragments; Field pH 7 (Raupach); 
	Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	REFER NOTES....
	Site Notes
	PHOTO NO; SURFACE - 16  (ROLL 4), THEMEDA TRIANDRA, TERMIUALRA VOLUCRIS, CHRYSOPOGN FALLAX, 
	E.POLYCARPA, CARISSA LANCEOLATA, E.CABBAGII, SELUMIA VER..., PLECTRACHUE PUNG..., TEROSOL, LEPTIC, 
	REGOLITHIC, PALIC,.....

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.8C	0.02A	1.96C	0.48	0.18	0.05	4.1K	2.7D	1.22
	5.8A
	0.2 - 0.3	4.6C	0.01A	0.49C	0.23	0.11	0.05	1.6K	0.9D	3.13
	5.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.85C	<2E	33.8A	54.4	5.6	4.2
	0.2 - 0.3	0.14C	<2E	39A	45.9	7.8	7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.2 - 0.3

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15B1_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B3	Total organic carbon - high frequency induction furnace, infrared
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method