Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	402	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	18/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 5067-4   1:50000	Rainfall:	No Data
	Northing/Long.:	8334028 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	670161  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Active, Severe (sheet) Active, Severe (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	34
	Silpanic Subnatric Brown Sodosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Sandy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Themeda triandra, Chrysopogon fallax
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Melaleuca viridiflora
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, , Sandstone
	Profile Morphology
	A11	0 - 0.02 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; 
	Non-sticky; Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to 
	- 
	A12	0.02 - 0.1 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy
	 (grains prominent) fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; 
	Non-plastic; Non-sticky; Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Clear, 
	Smooth change to - 
	A2	0.1 - 0.6 m	Brownish yellow (10YR6/6-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy
	 (grains prominent) fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; 
	Non-plastic; Non-sticky; Field pH 7 (Raupach); Common, very fine (0-1mm) roots; Sharp, Smooth
	 change to - 
	B2g	0.6 - 0.61 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sandy loam; Strong grade of structure, 20-50 
	mm, Angular blocky; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 
	Dry; Non-plastic; Slightly sticky; Fragipan, Moderately cemented, Continuous, Vesicular; Field pH
	 8 (Raupach); Sharp, Smooth change to - 
	B2q	0.61 - 0.65 m	Dark yellowish brown (10YR4/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; 
	Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; 
	Slightly sticky; Common (10 - 20 %), Ferromanganiferous, , Nodules; , Massive; Field pH 8.5 
	(Raupach); Sharp, Smooth change to - 
	B2k	0.65 -  m	Light yellowish brown (10YR6/4-Moist); ; Sandy clay loam; Dry; Moderately plastic; Normal 
	plasticity; Moderately sticky; Few cutans, <10% of ped faces or walls coated, distinct; Common
	 (10 - 20 %), Ferromanganiferous, , Nodules; Field pH 10 (Raupach); 
	Morphological Notes
	Observation Notes
	CLIFF'S STUDY SITE OF AN EROSION PROCESS..REFER NOTES
	Site Notes

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	402	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	PHOTO NO; SURFACE - 18,19,20,21,22 (ROLL 4), PROFILE - 17 (ROLL 51).....

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	402	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	4.6C	0.02A
	5.5A
	0.6 - 0.65	7.4C	0.38A
	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.6 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.6 - 0.65

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	402	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1