Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	18/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 5067-4   1:50000	Rainfall:	No Data
	Northing/Long.:	8333307 AMG zone: 52	Runoff:	No Data
	Easting/Lat.:	670812  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Pediment
	1-3%
	Morph. Type:	No Data	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	31
	Haplic Eutrophic Brown Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Themeda triandra, Iseilema vaginiflorum, 
	Astrebla squarrosa
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	20-50%, bouldery, 600mm-2m, rounded, Sandstone; 20-50%, bouldery, 600mm-2m, rounded, Sandstone
	Profile Morphology
	A11	0 - 0.03 m	Dark reddish brown (5YR3/2-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 5-10 mm, 
	Platy; Rough-ped fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Slightly plastic; Normal plasticity; Slightly sticky; 2-10%, fine gravelly, 2-
	6mm, rounded, Sandstone, coarse fragments; Field pH 7.5 (Raupach); Common, very fine (0-
	1mm) roots; Abrupt, Smooth change to - 
	A12	0.03 - 0.25 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Medium clay; Moderate grade of structure, 20-50 
	mm, Subangular blocky; Rough-ped fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) 
	Very fine (0.075-1mm) macropores, Dry; Very plastic; Normal plasticity; Very sticky; 10-20%, 
	cobbly, 60-200mm, rounded, Sandstone, coarse fragments; Field pH 7 (Raupach); Common, 
	very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B21	0.25 - 0.6 m	Dark reddish brown (2.5YR3/4-Moist); , 0-0% ; Medium heavy clay; Strong grade of structure, 
	2-5 mm, Subangular blocky; Strong grade of structure, 20-50 mm, Subangular blocky; Smooth-
	ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very plastic; Normal
	 plasticity; Non-sticky; Many cutans, >50% of ped faces or walls coated, distinct; Very few (0 -
	 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules; Field pH 6.5 (Raupach); Few, very fine 
	(0-1mm) roots; Clear, Smooth change to - 
	B22	0.6 -  m	Dark red (2.5YR3/6-Moist); , 0-0% ; Heavy clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Strong grade of structure, 20-50 mm, Subangular blocky; Smooth-ped 
	fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very plastic; Normal 
	plasticity; Moderately sticky; Many cutans, >50% of ped faces or walls coated, distinct; Field pH
	 6.5 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	PHOTO NO; SURFACE - 2.  FLINDERS GRASS,...., E.CABBAGII....REFER NOTES

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.7C	0.03A
	6.4A
	0.25 - 0.4	5.5C	0.02A	7.34C	2.24	0.54	0.04	14.1K	10.2D	0.28
	6.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.25 - 0.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.25 - 0.4

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15B1_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15B1_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1