Project Name:
	Project Code:	GEC	Site ID:	A185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.G. Tiller	Locality:	Grey
	Date Desc.:	07/06/55	Elevation:	150 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	140.543611111	Runoff:	Rapid
	Easting/Lat.:	-37.542777777	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-10%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	122 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Black earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.38 m	; Loam; 20-50%, bouldery, 600mm-2m, Basalt, coarse fragments; Gradual change to - 
	0.51 - 0.76 m	; Clay loam; 
	0.76 - 1.22 m	; Sandy clay; Gradual change to - 
	1.22 - 1.45 m	; Sandy clay; Gradual change to - 
	1.45 - 1.78 m	; Sandy clay; 
	2.03 - 2.44 m	; 
	2.44 - 3.96 m	; 
	4.27 - 5.18 m	; 
	5.18 -  m	; 
	Morphological Notes
	Weathering basalt - many hard lumps.
	Observation Notes
	Samples taken from sloping face of the quarry. Surface is suspect because of farming and later quarrying; 50cm & below is 
	definitely undisturbed. Weathering basalt at 36cm, 43cm, 20-33cm
	Site Notes
	Cleared farm land in use for quarrying road metal.

	Project Name:
	Project Code:	GEC	Site ID:	A185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.38	6.5A
	0.51 - 0.76
	0.76 - 1.22	7A
	1.22 - 1.45
	1.45 - 1.78	7.5A
	2.03 - 2.44
	2.44 - 3.96
	4.27 - 5.18
	5.18 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.38	0.3F	0.16B	0.58B	12C	41	34	13
	0.51 - 0.76	0.12F	0.19B	0.52B	10C	24	46	21
	0.76 - 1.22	0.079F	0.054B	0.26B	5C	25	44	25
	1.22 - 1.45	3C	26	50	22
	1.45 - 1.78	0.19F	0.023B	0.26B	9C	24	54	14
	2.03 - 2.44	0.5F	0.01B	0.22B	13C	32	48	8
	2.44 - 3.96	0C	0	0	0
	4.27 - 5.18	0.45F	0.27B	0C	0	0	0
	5.18 - 	0.44F	0.64B	0C	0	0	0
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.38
	0.51 - 0.76
	0.76 - 1.22
	1.22 - 1.45
	1.45 - 1.78
	2.03 - 2.44
	2.44 - 3.96
	4.27 - 5.18
	5.18 - 

	Project Name:
	Project Code:	GEC	Site ID:	A185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12_NR_CU	Total element - Cu(mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12_NR_ZN	Total element - Zn(mg/kg) - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	4A1	pH of 1:5 soil/water suspension
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	TE_NR_AL	Total Element Al - Not recorded
	TE_NR_CA	Total Element Ca - Not recorded
	TE_NR_MG	Total Element Mg - Not recorded
	TE_NR_NA	Total Element Na - Not recorded