Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BER2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	06/03/97	Elevation:	50 metres
	Map Ref.:	Sheet No. : 7029   1:100000	Rainfall:	No Data
	Northing/Long.:	6209776 AMG zone: 54	Runoff:	No runoff
	Easting/Lat.:	463619  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.1 m deep,Porous, Eolian 
	sand 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Dunefield
	Morph. Type:	Closed Depression	Relief:	5 metres
	Elem. Type:	Swale	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Subpeaty Lithocalcic Calcarosol Thick Non-gravelly Loamy 	Principal Profile Form:	N/A
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.2 m	Brown (7.5YR4/2-Moist); , 5YR46, 2-10% , 5-15mm, Faint; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; 
	Slightly plastic; Normal plasticity; Slightly sticky; Field pH 8.5 (Raupach); Many, fine (1-2mm) 
	roots; Clear, Smooth change to - 
	A12	0.2 - 0.45 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Fine sandy loam; Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Slightly plastic; 
	Normal plasticity; Slightly sticky; Field pH 10 (Raupach); Common, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B2k	0.45 - 1.1 m	Pink (7.5YR7/4-Moist); , 5YR58, 2-10% , 5-15mm, Distinct; Fine sandy clay loam; Massive grade 
	of structure; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Moderately plastic; Normal plasticity; 
	Slightly sticky; 10-20%, medium gravelly, 6-20mm, rounded tabular, dispersed, Calcrete, coarse 
	fragments; Common (10 - 20 %), Calcareous, Medium (2 -6 mm), Soft segregations; Field pH 10 
	(Raupach); Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	Dkm	1.1 -  m	; Fine sandy clay loam; Massive grade of structure; Earthy fabric; Wet; Calcrete, Moderately 
	cemented, Continuous, Massive; Field pH 10 (Raupach); 
	Morphological Notes
	Observation Notes
	Same location as Ber1, swale of duneplain
	Site Notes
	Berridale irrigated woodlot, Riverland, E. grandis planting failed, wet low lying site ponded water in winter

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BER2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BER2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile