Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A580	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:	COUNTRY BURNT A FEW YARDS AWAY
	Date Desc.:	24/09/58	Elevation:	 100 metres
	Map Ref.:	Sheet No. : SJ54-2   1:250000	Rainfall:	560
	Northing/Long.:	140.8772222	Runoff:	Slow
	Easting/Lat.:	-36.82944444	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	3 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, . *Species includes - Eucalyptus baxteri, Eucalyptus fastigata, Eucalyptus viminalis
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Grey (10YR5/1-Moist); ; Sand; , Granular; Weak consistence; Slightly plastic; Common
	0.03 - 0.08 m	Light brownish grey (10YR6/2-Moist); Very pale brown (10YR8/3-Moist); ; Sand; , Granular; Weak 
	consistence; Slightly plastic; Common, fine (1-2mm) roots; Diffuse change to - 
	0.08 - 0.2 m	Very pale brown (10YR8/3-Moist); Light brownish grey (10YR6/2-Moist); ; Sand; Loose 
	consistence; Common, fine (1-2mm) roots; Diffuse change to - 
	0.2 - 0.4 m	Pale brown (10YR6/3-Moist); Brownish yellow (10YR6/6-Moist); ; Sand; Loose consistence; 
	CommonDiffuse change to - 
	0.5 - 0.6 m	Pale brown (10YR6/3-Moist); Reddish yellow (5YR7/6-Moist); ; Sand; 20-50%, coarse gravelly, 
	20-60mm, Gravel, coarse fragments; CommonClear change to - 
	0.6 - 0.65 m	Light reddish brown (2.5YR6/4-Moist); ; Sand; Loose consistence; 0-2%, coarse gravelly, 20-
	60mm, Gravel, coarse fragments; Clear, Irregular change to - 
	0.7 - 0.85 m	Brownish yellow (10YR6/6-Moist); Red (10R5/6-Moist); ; Medium clay; Very firm consistence; 
	0.85 - 1.08 m	Red (10R5/6-Moist); Light olive grey (5Y6/2-Moist); ; Sandy medium clay; Very firm consistence; 
	1.08 - 1.31 m	Yellow (10YR7/6-Moist); Light red (2.5YR6/6-Moist); ; Sandy medium clay; Very firm 
	consistence; 
	1.31 - 1.64 m	Yellow (10YR7/6-Moist); Yellow (2.5Y8/6-Moist); , 0-2% ; , 0-2% ; Sandy medium clay; Very firm 
	consistence; 
	1.64 - 1.91 m	Light grey (10YR7/1-Moist); Pale olive (5Y6/3-Moist); ; Sandy medium clay; Very weak 
	consistence; Common (10 - 20 %), Calcareous, , Concretions; 
	1.91 - 2.03 m	Light grey (10YR7/1-Moist); Pale olive (5Y6/3-Moist); ; Sandy medium clay; Very weak 
	consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A580	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	CO. MACDONNELL Div. Soils Div. Report 4/65 p38 & S & L.U. No. 45

	Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A580	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.4H	 0.009C
	0.03 - 0.08	6.7H	 0.008C
	0.08 - 0.2	6.6H	 0.007C
	0.2 - 0.4	7H	 0.005C
	0.5 - 0.6	7H	 0.006C
	0.6 - 0.65	7.3H	 0.008C
	0.7 - 0.85	7.1H	 0.019C
	0.85 - 1.08	6.8H	 0.021C
	1.08 - 1.31	6.5H	 0.024C
	1.31 - 1.64	7.3H	 0.032C
	1.64 - 1.91	8.6H	 0.087C
	1.91 - 2.03
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.049B	 67C	 29	 1	 2
	0.03 - 0.08
	0.08 - 0.2	 64C	 33	 0	 2
	0.2 - 0.4
	0.5 - 0.6	29
	0.6 - 0.65
	0.7 - 0.85
	0.85 - 1.08	 40C	 24	 0	 34
	1.08 - 1.31
	1.31 - 1.64
	1.64 - 1.91	 3C	7
	1.91 - 2.03
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.08
	0.08 - 0.2
	0.2 - 0.4
	0.5 - 0.6
	0.6 - 0.65
	0.7 - 0.85
	0.85 - 1.08
	1.08 - 1.31
	1.31 - 1.64
	1.64 - 1.91
	1.91 - 2.03

	Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A580	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded