Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	30/10/88	Elevation:	296 metres
	Map Ref.:	Sheet No. : 6629-18   1:10000	Rainfall:	No Data
	Northing/Long.:	6216010 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	289360  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Shale 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	5 % 	Aspect:	40 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.06 m	Dark reddish brown (5YR3/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; Field pH 6 (Raupach); 
	A12	0.06 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; Field pH 6 (Raupach); Clear, Smooth change to - 
	A12	0.1 - 0.18 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; Field pH 6 (Raupach); Abrupt, Smooth change to - 
	B21	0.18 - 0.2 m	Dark reddish brown (2.5YR3/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, prominent; Field pH 7 (Raupach); 
	B21	0.2 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, prominent; Field pH 7.5 (Raupach); Clear, Smooth change to - 
	B22	0.3 - 0.4 m	Dark reddish brown (2.5YR3/3-Moist); , 2.5YR36, 20-50% , 0-5mm, Faint; Heavy clay; Moderate 
	grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Many
	 cutans, >50% of ped faces or walls coated, prominent; Field pH 8 (Raupach); 
	B22	0.4 - 0.48 m	Dark reddish brown (2.5YR3/3-Moist); , 2.5YR36, 20-50% , 15-30mm, Faint; Heavy clay; Moderate
	 grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 2-
	10%, coarse gravelly, 20-60mm, rounded platy, reoriented, Shale, coarse fragments; Many 
	cutans, >50% of ped faces or walls coated, prominent; Field pH 8 (Raupach); Abrupt, Smooth 
	change to - 
	B23k	0.48 - 0.5 m	Reddish brown (2.5YR4/4-Moist); , 2.5YR56, 20-50% , 15-30mm, Distinct; Heavy clay; Moderate 
	grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Many
	 cutans, >50% of ped faces or walls coated, prominent; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.5 (Raupach); 
	B23k	0.5 - 0.6 m	Reddish brown (2.5YR4/4-Moist); , 2.5YR56, 20-50% , 15-30mm, Distinct; Heavy clay; Moderate 
	grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Many
	 cutans, >50% of ped faces or walls coated, prominent; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.5 (Raupach); Abrupt, Smooth change to - 

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	C	0.6 - 0.8 m	; Weak grade of structure; Smooth-ped fabric; Dry; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.5 (Raupach); 
	Morphological Notes
	A11	Profile: Carbonate accumulation within the solum (contrast with A1233).
	B21	B horizon is finely structured at the top and coarsens noticeably
	B23k	Carbonates present
	B23k	Carbonates present
	C	The C horizon is the same as A1233,  banded and having grey, white and yellow 
	weathered WF Shale with a few carbonate bands.
	Observation Notes
	Site Notes

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06
	0.06 - 0.1
	0.1 - 0.18
	0.18 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.48
	0.48 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.06 - 0.1
	0.1 - 0.18
	0.18 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.48
	0.48 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.1
	0.1 - 0.18
	0.18 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.48
	0.48 - 0.5
	0.5 - 0.6
	0.6 - 0.8

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile