Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1276	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	01/11/88	Elevation:	No Data
	Map Ref.:	Sheet No. : 6629-18   1:10000	Rainfall:	No Data
	Northing/Long.:	6216540 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	290250  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam, fine sandy; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Dry; Strong consistence; Field pH 6 (Raupach); Sharp 
	change to - 
	B21	0.1 - 0.2 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Moderate grade of structure, 10-20 mm, 
	Polyhedral; Rough-ped fabric; Dry; Very strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Field pH 7 (Raupach); Clear change to - 
	B22	0.2 - 0.3 m	Red (2.5YR4/6-Moist); ; Heavy clay; Weak grade of structure, 20-50 mm, Angular blocky; Rough-
	ped fabric; Dry; Very strong consistence; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 8 (Raupach); 
	B22	0.3 - 0.4 m	Red (2.5YR4/6-Moist); ; Heavy clay; Weak grade of structure, 20-50 mm, Angular blocky; Rough-
	ped fabric; Dry; Very strong consistence; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 8 (Raupach); Clear change to - 
	B31	0.4 - 0.5 m	Red (2.5YR5/6-Moist); , 2.5YR54, 20-50% , 30-mm, Faint; Heavy clay; Weak grade of structure, 
	10-20 mm, Angular blocky; Rough-ped fabric; Dry; Very strong consistence; Few cutans, <10% 
	of ped faces or walls coated, faint; Common (10 - 20 %), Calcareous, Fine (0 - 2 mm), Soft 
	segregations; Field pH 8.5 (Raupach); 
	B32	0.5 - 0.7 m	Reddish yellow (5YR6/6-Moist); ; Heavy clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Rough-ped fabric; Dry; Very strong consistence; 20-50%, coarse gravelly, 20-60mm, 
	angular platy, undisturbed, Shale, coarse fragments; Few cutans, <10% of ped faces or walls 
	coated, faint; Common (10 - 20 %), Calcareous, Fine (0 - 2 mm), Soft segregations; Field pH 8.5
	 (Raupach); Gradual change to - 
	BC	0.7 - 1.3 m	Reddish yellow (5YR6/6-Moist); ; Heavy clay; Massive grade of structure; Rough-ped fabric; Many
	 (20 - 50 %), Calcareous, Fine (0 - 2 mm), Soft segregations; Field pH 8.5 (Raupach); Gradual 
	change to - 
	1.3 -  m	; Massive grade of structure; 
	Morphological Notes
	A1	Shallow, tough and degraded A1 (eroded?).  No high carbonate layer.
	B22	Massive very pedal B22 - sodic and high boron?  Very low sorptivity and no swelling in 
	the tough and shiny B2.
	BC	WFS is pale at depth (not the  gun-barrel grey of other locations).

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1276	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Observation Notes
	Site Notes

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1276	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.16C	0.25A
	7.36A
	0.1 - 0.2	7.03C	0.19A
	7.49A
	0.2 - 0.3	7.9C	0.32A
	8.5A
	0.3 - 0.4
	0.4 - 0.5	8.19C	0.47A
	9.04A
	0.5 - 0.7	8.49C	0.84A
	9.18A
	0.7 - 1.3
	1.3 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 1.3
	1.3 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 1.3
	1.3 - 

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1276	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour