Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A80	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:	TO BE CLEARED FOR SUB-CLOVER PASTURE
	Date Desc.:	08/06/54	Elevation:	 100 metres
	Map Ref.:	1:250000	Rainfall:	500
	Northing/Long.:	140.5825	Runoff:	Moderately rapid
	Easting/Lat.:	-36.4619444444445	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Calcic Yellow Chromosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Mid Strata - , , . *Species includes - Hakea species
	Tall Strata - Tree mallee, 0.51-1m, Sparse. *Species includes - Melaleuca unicinata
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; 
	0.08 - 0.15 m	Light yellowish brown (10YR6/4-Moist); ; Sandy loam; 
	0.15 - 0.23 m	Yellowish red (5YR5/6-Moist); , 10YR54; , 10YR78; Sandy medium clay; , Columnar; 
	0.23 - 0.3 m	Light yellowish brown (10YR6/4-Moist); , 5YR56; Sandy medium clay; Firm consistence; 
	0.41 - 0.46 m	Brownish yellow (10YR6/6-Moist); ; Sandy medium clay; Firm consistence; 
	0.56 - 0.66 m	Brownish yellow (10YR6/6-Moist); ; Sandy medium clay; Very weak consistence; , Calcareous, , 
	Soft segregations; 
	0.91 - 1.02 m	Brownish yellow (10YR6/6-Moist); ; Sandy medium clay; Massive grade of structure; Very weak 
	consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	BUCKINGHAM

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A80	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8A	 0.039C	 2.1F	 1.5	 0.18	 0.84
	0.08 - 0.15	6A	 0.026C
	0.15 - 0.23	6.1A	 0.047C	 5F	 9.1	 0.45	 0.79
	0.23 - 0.3	6.1A	 0.064C
	0.41 - 0.46	7.1A	 0.15C
	0.56 - 0.66	9A	 0.43C
	0.91 - 1.02	9A	 0.49C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.004F	 0.12B	 27C	 54	 5	 13
	0.08 - 0.15
	0.15 - 0.23	 0.007F	 0.48B	 16C	 31	 0	 53
	0.23 - 0.3
	0.41 - 0.46
	0.56 - 0.66
	0.91 - 1.02
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.23
	0.23 - 0.3
	0.41 - 0.46
	0.56 - 0.66
	0.91 - 1.02

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A80	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded