Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:	SITE CLEARED
	Date Desc.:	08/06/54	Elevation:	 100 metres
	Map Ref.:	1:250000	Rainfall:	500
	Northing/Long.:	140.552222222222	Runoff:	Very slow
	Easting/Lat.:	-36.4394444444445	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	9 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Yellow Chromosol     	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Mid Strata - , , . *Species includes - Eucalyptus baxteri
	Tall Strata - , , . *Species includes - Eucalyptus leptophleba, Banksia marginata, Xanthorrhoea australis
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Grey (10YR6/1-Moist); ; Sand; 
	0.08 - 0.15 m	Grey (10YR6/1-Moist); ; Sand; 
	0.15 - 0.33 m	Light grey (10YR7/1-Moist); ; Sand; 
	0.33 - 0.41 m	Light yellowish brown (10YR6/4-Moist); ; Clayey sand; , Columnar; 
	0.51 - 0.61 m	Brownish yellow (10YR6/6-Moist); , 10R56; Sandy clay loam; Very firm consistence; 
	0.74 - 0.86 m	Yellow (10YR7/6-Moist); , 10R63; Sandy clay loam; Massive grade of structure; Very firm 
	consistence; 
	1.02 - 1.12 m	Yellow (10YR7/6-Moist); , 10R66; , 10YR61; Sandy clay loam; Very firm consistence; 
	Morphological Notes
	Observation Notes
	LAYERS RENUMBERED 10/11/92                                                                                              
	Site Notes
	BUCKINGHAM

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.5A	 0.011C	 2.3F	 0.3	 0.11	 0.04
	0.08 - 0.15
	0.08 - 0.33	7.1A	 0.012C
	0.33 - 0.41	6.9A	 0.016C	 8.2F	 4.4	 0.92	 0.34
	0.51 - 0.61	6.9A	 0.017C
	0.74 - 0.86	6.5A	 0.028C
	1.02 - 1.12	6.3A	 0.046C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.002F	 0.03C	 0.02B	 16C	 79	 2	 2
	0.08 - 0.15
	0.08 - 0.33	 0.021A
	0.33 - 0.41	 0.006F	 0.056C	 0.36B	 5C	 39	 0	 55
	0.51 - 0.61	 0.016A	 3C	 58	 1	 37
	0.74 - 0.86	 0.009A	 3C	 65	 1	 29
	1.02 - 1.12	 0.01A	 2C	 68	 0	 29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.08 - 0.33
	0.33 - 0.41
	0.51 - 0.61
	0.74 - 0.86
	1.02 - 1.12

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded