Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	028	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	15/11/90	Elevation:	408 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6152480 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	313625  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.5 m deep,Porous, Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	2 metres
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	1 % 	Aspect:	30 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	O	0 - 0.04 m	Organic Layer; Dark brown (7.5YR3/2-Moist); , 0-0% ; Sandy loam; Single grain grade of 
	structure; Loose consistence; Sharp, Smooth change to - 
	A1	0.04 - 0.2 m	Brown (7.5YR4/2-Moist); , 0-0% ; Sandy loam; Single grain grade of structure; Loose 
	consistence; Gradual, Smooth change to - 
	A2	0.2 - 0.5 m	Light reddish brown (2.5YR6/4-Moist); White (10YR8/1-Dry); , 0-0% ; Sandy loam; Single grain 
	grade of structure; Loose consistence; Abrupt, Smooth change to - 
	Bt	0.5 - 0.7 m	Brownish yellow (10YR6/8-Moist); , 10YR36, 10-20% , 5-15mm, Distinct; Light clay; Single grain
	 grade of structure; Loose consistence; Clear, Smooth change to - 
	Bt	0.7 - 1.2 m	Yellowish brown (10YR5/8-Moist); , 10YR62, 10-20% , 5-15mm, Distinct; , 5YR58; Light medium
	 clay; Single grain grade of structure; Loose consistence; Clear, Smooth change to - 
	Bt	1.2 - 1.5 m	Yellowish brown (10YR5/4-Moist); , 10YR58, 10-20% , 5-15mm, Distinct; Sandy clay; Single 
	grain grade of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	028	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	028	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile