Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	039	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	27/11/90	Elevation:	419 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6158160 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	319310  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1 m deep,Porous, Clay 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Peneplain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	0.5 % 	Aspect:	20 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy3.13
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sod grass, <0.25m, Mid-dense. *Species includes - Danthonia species, Hordeum marineum
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A	0 - 0.25 m	Brown (10YR5/3-Moist); Light grey (10YR7/1-Dry); , 0-0% ; Clayey sand; Single grain grade of 
	structure; Dry; Loose consistence; Sharp change to - 
	Btg	0.25 - 0.35 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sandy clay; Single grain grade of structure; Loose 
	consistence; Clear change to - 
	Btg	0.35 - 0.4 m	Greyish brown (10YR5/2-Moist); , 0-0% ; Sandy clay loam; Single grain grade of structure; Moist; 
	Loose consistence; Clear change to - 
	Bt	0.4 - 0.5 m	Olive grey (5Y5/2-Moist); , 7.5YR58, 10-20% , 5-15mm, Distinct; Sandy clay; Single grain grade 
	of structure; Wet; Loose consistence; Clear change to - 
	Btk	0.5 - 0.7 m	Olive grey (5Y5/2-Moist); , 7.5YR58, 10-20% , 5-15mm, Distinct; Light clay; Single grain grade of
	 structure; Loose consistence; Gradual change to - 
	Bt	0.7 - 0.9 m	Olive grey (5Y5/2-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; Sandy clay; Single grain grade 
	of structure; Loose consistence; 
	Bt	0.9 - 1.1 m	Dark greyish brown (2.5Y4/2-Moist); , 0-0% ; Silty clay; Single grain grade of structure; Loose 
	consistence; 
	C	1.1 - 1.5 m	Light olive grey (5Y6/2-Moist); , 2.5YR66, 0-0% ; Clay loam, sandy; Single grain grade of 
	structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	039	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	039	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile