Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	064	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/12/90	Elevation:	423 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6155000 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	314950  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 1.4 m deep,Porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	1 % 	Aspect:	350 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.11
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Confidence level not specified	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, rounded tabular, Ironstone
	Profile Morphology
	O	0 - 0.01 m	Organic Layer; , 0-0% ; Single grain grade of structure; Fine, (0 - 5) mm crack; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Loose consistence; Abrupt, Smooth change 
	to - 
	A1	0.01 - 0.1 m	Dark yellowish brown (10YR4/4-Moist); Light brown (7.5YR6/4-Dry); , 0-0% ; Loamy sand; 
	Massive grade of structure; Moderately moist; Firm consistence; Abrupt, Wavy change to - 
	A2	0.1 - 0.3 m	Strong brown (7.5YR5/6-Moist); Pink (5YR7/4-Dry); , 0-0% ; Loamy sand; Single grain grade of 
	structure; Moist; Loose consistence; Sharp, Wavy change to - 
	Bt	0.3 - 0.5 m	Reddish brown (5YR5/4-Moist); Pink (5YR7/4-Dry); , 2.5YR58, 20-50% , 5-15mm, Distinct; 
	Medium clay; Moderate grade of structure; Wet; Loose consistence; Clear, Wavy change to - 
	BC	0.5 - 0.9 m	Strong brown (7.5YR5/8-Moist); Yellow (10YR7/6-Dry); , 10R46, 20-50% , 5-15mm, Prominent; 
	Light clay; Single grain grade of structure; Loose consistence; Clear, Tongued change to - 
	C1r	0.9 - 1 m	Very pale brown (10YR7/4-Moist); Very pale brown (10YR7/4-Dry); , 10YR68, 20-50% , 5-15mm, 
	Prominent; , 10R46; Light clay; Abrupt, Tongued change to - 
	C1	1 - 1.4 m	Very pale brown (10YR7/4-Moist); Very pale brown (10YR7/4-Dry); , 10YR68, 20-50% , 5-15mm, 
	Prominent; , 10R46; Light clay; Single grain grade of structure; Loose consistence; Abrupt, 
	Tongued change to - 
	C2r	1.4 - 2.3 m	White (5YR8/1-Moist); White (5YR8/1-Dry); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 10R46; 
	Fine sandy clay; Single grain grade of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	A1423

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	064	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.7C	0.05A	1.72D	0.71	0.15	0.1	4K	2.7D	2.50
	4.9A
	0.1 - 0.3	4.3C	0.05A	1.02D	1.15	0.13	0.14	3.9K	2.4D	3.59
	4.5A
	0.3 - 0.5	4.4C	0.07A	1.85D	5.55	0.21	0.4	0.72A	11.1K	8D	3.60
	4.7A
	0.5 - 1	4.5C	0.06A	1.01D	5.21	0.11	0.4	0.52A	9K	6.7D	4.44
	4.6A
	1 - 2.3	4C	0.08A	0.07D	0.98	0.06	0.21	4.44A	4.4K	1.3D	4.77
	3.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.3C	5E	0.028D	44B	46	4	5
	0.1 - 0.3	0.9C	3E	0.023D	41B	31	6	22
	0.3 - 0.5	0.6C	0D	9B	10	8	71
	0.5 - 1	0.2C	0D	13B	13	13	60
	1 - 2.3	0.1C	0D	26B	26	12	37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.5
	0.5 - 1
	1 - 2.3

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	064	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15B2_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette