Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	065	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/12/90	Elevation:	437 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6155040 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	315260  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 1.3 m deep,Porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	15 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Moderate (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.11
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, rounded tabular, Ironstone
	Profile Morphology
	A	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); Light grey (10YR7/1-Dry); , 0-0% ; Single grain grade of 
	structure; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores,
	 Dry; Very weak consistence; Clear, Smooth change to - 
	A1	0.1 - 0.2 m	Very dark greyish brown (10YR3/2-Moist); Grey (10YR5/1-Dry); , 0-0% ; Fine sand; Massive grade 
	of structure; Moderately moist; Loose consistence; Clear, Smooth change to - 
	A2	0.2 - 0.3 m	Brown (10YR4/3-Moist); Light grey (10YR7/2-Dry); , 7.5YR58, 0-2% , 0-5mm, Faint; Weak grade 
	of structure; Moist; Loose consistence; Sharp, Smooth change to - 
	Bt	0.3 - 0.4 m	Very pale brown (10YR7/3-Moist); Yellowish brown (10YR5/4-Dry); , 2.5YR46, 2-10% , 5-15mm, 
	Distinct; , 7.5YR58; Loam; Moderate grade of structure; Wet; Weak consistence; Clear, Wavy 
	change to - 
	Bt	0.4 - 0.5 m	Strong brown (7.5YR5/8-Moist); , 10YR63, 2-10% , 5-15mm, Distinct; , 2.5R48; Clear, Wavy 
	change to - 
	Bt	0.5 - 0.7 m	Strong brown (7.5YR5/8-Moist); , 10YR63, 2-10% , 5-15mm, Distinct; , 2.5R48; Strong grade of 
	structure; Weak consistence; Clear, Wavy change to - 
	BC	0.7 - 1 m	Light brownish grey (2.5Y6/2-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; Loam; Single 
	grain grade of structure; Loose consistence; Clear, Irregular change to - 
	C	1 - 1.3 m	Light grey (2.5Y7/2-Moist); , 7.5YR58, 10-20% , 15-30mm, Prominent; Loam; Single grain grade 
	of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	A1424

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	065	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5C	0.1A	3.93D	1.17	0.16	0.21	6.2K	5.5D	3.39
	5A
	0.1 - 0.3	4.8C	0.06A	3.1D	1.03	0.12	0.12	5.8K	4.4D	2.07
	4.9A
	0.3 - 0.4	4.6C	0.06A	3.16D	3.63	0.21	0.29	0.35A	10.2K	7.3D	2.84
	4.9A
	0.4 - 0.5	4.7C	0.06A	2.67D	4.5	0.14	0.31	0.11A	9.8K	7.6D	3.16
	4.9A
	0.5 - 1	4.4C	0.07A	1.66D	5.56	0.12	0.43	0.4A	9.9K	7.8D	4.34
	4.7A
	1 - 1.3	3.9C	0.09A	0.95D	5.92	0.14	0.57	2.16A	10.9K	7.6D	5.23
	4.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.8C	6E	0.05D	48B	38	5	9
	0.1 - 0.3	1.2C	7E	0.041D	46B	39	8	9
	0.3 - 0.4	0.9C	0D	19B	11	8	60
	0.4 - 0.5	0.4C	0D	13B	12	8	66
	0.5 - 1	0.3C	0D	18B	20	10	50
	1 - 1.3	0.3C	0D	23B	20	13	43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 1
	1 - 1.3

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	065	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15B2_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette