Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	068	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/12/90	Elevation:	430 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6155040 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	315650  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 2 m deep,Porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.32
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Dark brown (7.5YR3/2-Moist); Brown (7.5YR5/2-Dry); , 0-0% ; Clear, Smooth change to - 
	A12	0.02 - 0.1 m	Dark brown (7.5YR3/2-Moist); Brown (7.5YR5/2-Dry); , 0-0% ; Sand; Single grain grade of 
	structure; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores,
	 Dry; Loose consistence; Clear, Smooth change to - 
	A13	0.1 - 0.2 m	Dark brown (7.5YR3/2-Moist); Brown (7.5YR5/2-Dry); , 0-0% ; Loam; Massive grade of structure; 
	Moderately moist; Loose consistence; Clear, Smooth change to - 
	A2	0.2 - 0.3 m	Light brownish grey (10YR6/2-Moist); White (10YR8/2-Dry); , 0-0% ; Weak grade of structure; 
	Moist; Loose consistence; Abrupt, Wavy change to - 
	AB	0.3 - 0.4 m	Light grey (10YR7/2-Moist); Light grey (10YR7/2-Dry); , 5YR58, 10-20% , 5-15mm, Distinct; 
	Moderate grade of structure; Wet; Loose consistence; Abrupt, Wavy change to - 
	Bt	0.4 - 0.5 m	Greyish brown (10YR5/2-Moist); Light brownish grey (10YR6/2-Dry); , 2.5YR46, 10-20% , 5-
	15mm, Prominent; , 5YR58; Loam; Single grain grade of structure; Loose consistence; Clear, 
	Wavy change to - 
	BC1	0.5 - 1 m	Pale red (2.5YR6/2-Moist); , 10YR66, 2-10% , 15-30mm, Faint; Sandy clay; Single grain grade of
	 structure; Loose consistence; Clear, Wavy change to - 
	BC2	1 - 1.1 m	Pale red (2.5YR6/2-Moist); , 10YR66, 2-10% , 15-30mm, Faint; Sandy clay; Clear, Wavy change 
	to - 
	C	1.1 - 1.9 m	Pale red (2.5YR6/2-Moist); , 10YR66, 0-2% , 0-5mm, Faint; Loose consistence; Gradual, Wavy 
	change to - 
	Cr	1.9 - 2 m	Weak red (2.5YR5/2-Moist); , 0-0% ; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	A1427

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	068	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	068	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.1	4.6C	0.07A	2.55D	0.91	0.16	0.16	5.2K	3.8D	3.08
	4.7A
	0.1 - 0.2	0.93D	0.37	0.07	0.11	2K	1.5D	5.50
	0.2 - 0.3	4.6C	0.05A
	4.5A
	0.3 - 0.4	4.5C	0.05A	0.68D	0.84	0.11	0.17	1.7K	1.8D	10.00
	4.6A
	0.4 - 0.5	4.6C	0.08A	2.56D	3.72	0.27	0.52	0.18A	8.6K	7.1D	6.05
	4.9A
	0.5 - 1.1	4.3C	0.15A	1.73D	4.26	0.3	0.69	0.39A	8.6K	7D	8.02
	4.5A
	1.1 - 2	4.2C	0.78A	0.33D	1.87	0.04	3.1	2.9K	5.3D	106.90
	4.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	13.7C	0.205D
	0.02 - 0.1	1.8C	7E	0.052D	54B	31	5	8
	0.1 - 0.2	56B	33	5	5
	0.2 - 0.3	0.6C	0.02D
	0.3 - 0.4	0.2C	0D	43B	34	6	16
	0.4 - 0.5	0.9C	0D	27B	22	7	45
	0.5 - 1.1	0.3C	0D	22B	21	9	45
	1.1 - 2	0.1C	0D	46B	32	7	14
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 1.1
	1.1 - 2

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	068	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15B2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15B2_K	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_MG	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15B2_NA	Exchangeable bases and CEC - 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15J_BASES	Sum of Bases
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette