Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	079	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	18/12/90	Elevation:	434 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6154410 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	318260  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 3 m deep,Porous, 
	Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Peneplain
	Morph. Type:	Open depression (vale)	Relief:	5 metres
	Elem. Type:	Footslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Gn2.9
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Confidence level not specified	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); Dark greyish brown (10YR4/2-Dry); , 0-0% ; Loamy 
	sand; Single grain grade of structure; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very 
	fine (0.075-1mm) macropores, Dry; Very weak consistence; Clear, Smooth change to - 
	A12	0.05 - 0.4 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); , 0-0% ; Loamy sand; Massive grade of
	 structure; Moderately moist; Loose consistence; Abrupt, Smooth change to - 
	A21	0.4 - 0.6 m	Pale brown (10YR6/3-Moist); Very pale brown (10YR7/4-Dry); , 0-0% ; Loamy sand; Weak grade 
	of structure; Moist; Loose consistence; Clear, Smooth change to - 
	A22	0.6 - 0.8 m	Light grey (10YR7/2-Moist); White (10YR8/2-Dry); , 7.5YR34, 0-2% , 0-5mm, Faint; Loamy sand; 
	Single grain grade of structure; Wet; Loose consistence; Sharp, Smooth change to - 
	AB	0.8 - 0.9 m	Dark greyish brown (10YR4/2-Moist); Greyish brown (10YR5/2-Dry); , 10YR58, 10-20% , 5-15mm, 
	Distinct; Clayey sand; Single grain grade of structure; Loose consistence; Clear, Smooth 
	change to - 
	Bt	0.85 - 1 m	Grey (10YR6/1-Moist); Grey (7.5YR6/0-Dry); , 7.5YR58, 20-50% , 5-15mm, Prominent; Clay loam, 
	sandy; Single grain grade of structure; Loose consistence; Smooth change to - 
	BCc	1 - 1.3 m	Light grey (10YR7/2-Moist); Light grey (10YR7/2-Dry); , 10YR68, 20-50% , 30-mm, Distinct; 
	Sandy clay loam; Single grain grade of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	079	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	079	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile