Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	094	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	20/12/90	Elevation:	425 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6157320 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	319915  Datum: AGD66	Drainage:	Very poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 1 m deep,Porous, 
	Sandstone 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Greyish brown (10YR5/2-Moist); White (10YR8/2-Dry); , 7.5YR56, 2-10% , 0-5mm, Faint; Loamy 
	sand; Single grain grade of structure; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Dry; Loose consistence; Non-plastic; Non-sticky; Field pH 7 
	(Raupach); Few, coarse (>5mm) roots; Sharp, Smooth change to - 
	A21	0.1 - 0.3 m	Greyish brown (10YR5/2-Moist); White (10YR8/1-Dry); , 7.5YR46, 2-10% , 0-5mm, Faint; Loamy 
	sand; Massive grade of structure; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Moderately moist; Loose consistence; Non-plastic; Non-sticky; Field 
	pH 7 (Raupach); Common, medium (2-5mm) roots; Clear, Smooth change to - 
	A22	0.3 - 0.5 m	Pale brown (10YR6/3-Moist); Very pale brown (10YR8/3-Dry); , 10YR68, 2-10% , 0-5mm, Faint; 
	Loamy sand; Weak grade of structure; Common (1-5 per 100mm2)  macropores, Moist; Loose 
	consistence; Non-plastic; Non-sticky; Few, very fine (0-1mm) roots; Sharp, Tongued change to - 
	Btg	0.5 - 0.65 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Dry); , 10YR66, 10-20% , 5-15mm, 
	Distinct; Light clay; Moderate grade of structure; Wet; Loose consistence; Very plastic; Normal 
	plasticity; Moderately sticky; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; 
	0.65 - 0.8 m	; Non-plastic; Non-sticky; 
	0.8 - 1 m	; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	094	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	094	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile