Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	29/04/91	Elevation:	412 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6157480 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	317010  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 3 m deep,Slightly 
	porous, Clay 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Peneplain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Level
	Slope:	0.5 % 	Aspect:	290 degrees
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sedge, 0.26-0.5m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); Light brownish grey (10YR6/2-Dry); , 0-0% ; Sandy loam; 
	Single grain grade of structure; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Very weak consistence; Clear, Smooth change to - 
	A12	0.1 - 0.3 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); , 10YR46, 0-2% , 0-5mm, Faint; Sandy 
	loam; Massive grade of structure; Common (1-5 per 100mm2)  macropores, Moderately moist; 
	Weak consistence; Clear, Smooth change to - 
	A2	0.3 - 0.45 m	Light yellowish brown (10YR6/4-Moist); Very pale brown (10YR7/3-Dry); , 10YR46, 0-2% , 0-5mm,
	 Faint; Loamy sand; Weak grade of structure; Moist; Loose consistence; Abrupt, Smooth 
	change to - 
	AB	0.45 - 0.5 m	Light grey (10YR7/2-Moist); White (10YR8/1-Dry); , 10YR68, 10-20% , 0-5mm, Distinct; , 
	10YR52; Clayey sand; Single grain grade of structure; Loose consistence; Sharp, Irregular 
	change to - 
	Bt	0.5 - 0.6 m	Grey (10YR6/1-Moist); Grey (10YR6/1-Dry); , 7.5YR58, 20-50% , 15-30mm, Distinct; , 10YR31; 
	Medium clay; Single grain grade of structure; Dry; Strong consistence; Clear, Wavy change to - 
	B	0.6 - 1 m	Light grey (10YR7/2-Moist); Light grey (10YR7/2-Dry); , 10YR68, 20-50% , 15-30mm, Distinct; 
	Light clay; Strong grade of structure; Dry; Very strong consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile