Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	102	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	23/04/91	Elevation:	394 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6155205 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	312360  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 1 m deep,Porous, 
	Clay 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	340 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:	Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.82
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 20.01-35m, Mid-dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; White (10YR8/1-Dry); , 0-0% ; Loamy sand; Single grain grade of structure; Fine, 
	(0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak 
	consistence; Non-plastic; Non-sticky; Field pH 7 (Raupach); Abundant, very fine (0-1mm) roots; 
	Sharp, Smooth change to - 
	A1	0.02 - 0.1 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); , 0-0% ; Loamy sand; Massive grade of
	 structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Loose 
	consistence; Non-plastic; Non-sticky; Field pH 7 (Raupach); Common, very fine (0-1mm) roots; 
	Clear, Smooth change to - 
	A2	0.1 - 0.5 m	Light brownish grey (10YR6/2-Moist); Light grey (2.5Y7/2-Dry); , 10YR76, 10-20% , 5-15mm, 
	Distinct; Sandy loam; Weak grade of structure; Moist; Firm consistence; Slightly plastic; Normal
	 plasticity; Slightly sticky; 0-2%, medium gravelly, 6-20mm, rounded, dispersedstrong, Ironstone,
	 coarse fragments; Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Abrupt, Wavy 
	change to - 
	B1	0.5 - 0.7 m	Yellowish brown (10YR5/8-Moist); Light grey (2.5Y7/2-Dry); , 10YR71, 20-50% , 5-15mm, 
	Distinct; Sandy clay loam; Single grain grade of structure; Wet; Loose consistence; Moderately 
	plastic; Normal plasticity; Slightly sticky; 2-10%, medium gravelly, 6-20mm, angular, 
	dispersedstrong, Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) 
	roots; Clear change to - 
	Bt	0.7 - 1 m	Yellowish brown (10YR5/4-Moist); , 2.5Y62, 20-50% , 5-15mm, Distinct; Light clay; Single grain 
	grade of structure; Moist; Loose consistence; Very plastic; Normal plasticity; Moderately sticky; 
	Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	102	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	102	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile