Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	25/04/91	Elevation:	420 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6157030 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	319020  Datum: AGD66	Drainage:	Very poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, 3 m deep,Porous, 
	Clay 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	1.5 % 	Aspect:	340 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR5/3-Moist); Light grey (10YR7/2-Dry); , 7.5YR32, 0-2% , 0-5mm, Faint; Loamy sand; 
	Single grain grade of structure; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Loose consistence; Non-plastic; Non-sticky; Field pH 6 (Raupach); 
	Many, very fine (0-1mm) roots; Clear change to - 
	AB	0.1 - 0.3 m	Light brownish grey (10YR6/2-Moist); White (10YR8/1-Dry); , 7.5YR32, 0-2% , 0-5mm, Distinct; 
	Heavy clay; Massive grade of structure; Moderately moist; Loose consistence; Non-plastic; Non-
	sticky; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Sharp change to - 
	Btg	0.3 - 0.4 m	Dark yellowish brown (10YR4/6-Moist); Yellowish brown (10YR5/6-Dry); , 10YR42, 20-50% , 0-
	5mm, Faint; Heavy clay; Weak grade of structure; Moist; Loose consistence; Very plastic; 
	Normal plasticity; Very sticky; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; Sharp change
	 to - 
	Btk	0.4 - 0.5 m	Light yellowish brown (2.5Y6/4-Moist); Light yellowish brown (2.5Y6/4-Dry); ; Medium heavy clay; 
	Moderate grade of structure; Wet; Very firm consistence; Very plastic; Normal plasticity; Very 
	sticky; Field pH 9 (Raupach); Common, very fine (0-1mm) roots; Sharp change to - 
	Btk	0.5 - 0.7 m	Greyish brown (2.5Y5/2-Moist); Light yellowish brown (2.5Y6/4-Dry); , 10YR76, 10-20% , 5-15mm,
	 Faint; Medium clay; Strong grade of structure; Strong consistence; Moderately plastic; Normal 
	plasticity; Moderately sticky; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field 
	pH 9 (Raupach); Few, fine (1-2mm) roots; Clear change to - 
	Bck	0.7 - 1 m	Light grey (2.5Y7/2-Moist); Light grey (2.5Y7/2-Dry); , 10YR68, 20-50% , 5-15mm, Distinct; Single
	 grain grade of structure; Moderately plastic; Normal plasticity; Slightly sticky; Field pH 9 
	(Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile