Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	23/07/91	Elevation:	464 metres
	Map Ref.:	Sheet No. : 6628-16   1:10000	Rainfall:	No Data
	Northing/Long.:	6161440 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	314620  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.6 m deep,Sand 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Alcove	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	30 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, No gully erosion (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Rudosol     	Principal Profile Form:	Uc1.41
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, rounded, Schist
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Sandy clay loam; Moderate grade of structure, Granular; 
	Earthy fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Weak consistence; Field pH 5.5 (Raupach, 0.05); Many, very fine (0-1mm) roots; Clear 
	change to - 
	A12	0.1 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 2-10% , Distinct; Sandy clay loam; Massive grade of 
	structure; Earthy fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Wet; Very weak consistence; Field pH 5.5 (Raupach, 0.2); Common, very fine (0-
	1mm) roots; Gradual change to - 
	A21	0.3 - 0.5 m	Brown (10YR5/3-Moist); , 2-10% , Faint; Sandy loam; Massive grade of structure; Earthy fabric; 
	Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Wet; Very 
	weak consistence; Field pH 6 (Raupach, 0.4); Common, very fine (0-1mm) roots; Clear change 
	to - 
	A22	0.5 - 0.65 m	Yellowish brown (10YR5/4-Moist); , 2-10% , Faint; Sandy loam; Massive grade of structure; 
	Earthy fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Wet; Very weak consistence; Field pH 6 (Raupach, 0.65); Few, very fine (0-1mm) roots; Clear 
	change to - 
	2A1	0.65 - 0.75 m	Dark grey (10YR4/1-Moist); , 10-20% , Distinct; Sandy clay loam; Massive grade of structure; 
	Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Weak consistence; Field pH 6 (Raupach, 0.7); Few, very fine (0-1mm) roots; Clear 
	change to - 
	2A1	0.75 - 1 m	Very pale brown (10YR7/3-Moist); , 2-10% , Distinct; Sand; Sandy (grains prominent) fabric; 
	Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Weak 
	consistence; Field pH 6 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	234	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile