Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	243	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	25/07/91	Elevation:	444 metres
	Map Ref.:	Sheet No. : 6628-16   1:10000	Rainfall:	No Data
	Northing/Long.:	6161725 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	315670  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1 m deep,Slightly porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	140 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, No sheet erosion (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	2-10%, stony, 200-600mm, angular tabular, Schist
	Profile Morphology
	A11	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, <2 mm, Granular; 
	Earthy fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Weak consistence; Field pH 5.5 (Raupach, 0.05); 
	A12	0.1 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Very weak consistence; Field pH 6 (Raupach, 0.2); 
	A21	0.3 - 0.5 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Wet; 
	Very weak consistence; Field pH 6 (Raupach, 0.4); 
	A22	0.5 - 0.7 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Wet; 
	Very weak consistence; 20-50%, medium gravelly, 6-20mm, angular, stratifiedstrong, Quartz, 
	coarse fragments; Field pH 6 (Raupach, 0.6); 
	Bt	0.7 - 0.8 m	Greyish brown (10YR5/2-Moist); , 10-20% , 5-15mm, Prominent; Medium heavy clay; Earthy 
	fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Firm consistence; Field pH 6 (Raupach, 0.75); 
	BC	0.8 - 1 m	Yellowish brown (10YR5/4-Moist); , 10-20% , 5-15mm, Distinct; Medium clay; Earthy fabric; Fine,
	 (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very 
	firm consistence; Field pH 6 (Raupach, 0.95); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	243	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	243	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile