Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	20/07/91	Elevation:	440 metres
	Map Ref.:	Sheet No. : 6628-16   1:10000	Rainfall:	No Data
	Northing/Long.:	6162040 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	316365  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.1 m deep,Slightly porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Open depression (vale)	Relief:	0 metres
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	100 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Fine, 
	(0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very weak 
	consistence; Field pH 5.5 (Raupach); Abundant, very fine (0-1mm) roots; 
	A1	0.1 - 0.3 m	Dark grey (5Y4/1-Moist); , 0-0% ; Loamy sand; Massive grade of structure; Fine, (0 - 5) mm crack; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Wet; Loose consistence; Field pH 
	5.5 (Raupach); Many, very fine (0-1mm) roots; 
	A2	0.3 - 0.5 m	Grey (5Y6/1-Moist); , 0-0% ; Sand; Massive grade of structure; Fine, (0 - 5) mm crack; Many (>5 
	per 100mm2) Very fine (0.075-1mm) macropores, Wet; Loose consistence; Field pH 6 
	(Raupach); Common, very fine (0-1mm) roots; 
	A2	0.5 - 0.6 m	Grey (5Y6/1-Moist); , 0-0% ; Sand; Massive grade of structure; Fine, (0 - 5) mm crack; Many (>5 
	per 100mm2) Very fine (0.075-1mm) macropores, Wet; Loose consistence; 10-20%, medium 
	gravelly, 6-20mm, angular, stratified, Quartz, coarse fragments; Field pH 7 (Raupach); Common, 
	very fine (0-1mm) roots; Sharp, Irregular change to - 
	Bt	0.6 - 0.85 m	Greyish brown (2.5Y5/2-Moist); , 10-20% , Distinct; Medium clay; Massive grade of structure; 
	Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Firm 
	consistence; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	C	0.85 - 1 m	Light yellowish brown (2.5Y6/4-Moist); , 20-50% , Prominent; Sandy clay loam; Massive grade of 
	structure; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores,
	 Moist; Very firm consistence; Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile