Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	257	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	01/08/91	Elevation:	450 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6159650 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	317430  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.6 m deep,Porous, Schist 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	10 % 	Aspect:	200 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, Moderate (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.21
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, angular, Quartz
	Profile Morphology
	O	0 - 0.03 m	Organic Layer; Dark grey (10YR4/1-Moist); , 0-0% ; Single grain grade of structure; Moist; Field 
	pH 6 (Raupach, 0.01); 
	A1	0.03 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Moist;
	 10-20%, stony, 200-600mm, angular tabular, dispersedstrong, Quartz, coarse fragments; Field 
	pH 5.5 (Raupach, 0.05); Many, very fine (0-1mm) roots; Clear change to - 
	A2	0.1 - 0.2 m	Brown (10YR5/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Moist; 10-20%, 
	stony, 200-600mm, angular tabular, dispersedstrong, Quartz, coarse fragments; Field pH 5.5 
	(Raupach, 0.15); Many, very fine (0-1mm) roots; Clear change to - 
	B1	0.2 - 0.3 m	Light red (5R6/6-Moist); , 0-0% ; Sandy clay; Field pH 5.5 (Raupach); Abrupt change to - 
	Bt	0.3 - 0.4 m	Red (2.5YR4/6-Moist); , 2-10% , Distinct; Medium heavy clay; Massive grade of structure; Moist; 
	Field pH 5.5 (Raupach, 0.3); Common, fine (1-2mm) roots; Clear change to - 
	BC	0.4 - 0.5 m	Brownish yellow (10YR6/8-Moist); , 10-20% , Distinct; Medium heavy clay; Massive grade of 
	structure; Moderately moist; Field pH 6 (Raupach, 0.45); Few, fine (1-2mm) roots; 
	BC	0.5 - 0.65 m	Brownish yellow (10YR6/8-Moist); , 10-20% , Distinct; Medium clay; Moderately moist; Field pH 6
	 (Raupach, 0.45); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	257	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	257	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile